Pset_SanitaryTerminalTypeUrinal

BACnet MVD

#### 7.6.4.15 Pset_SanitaryTerminalTypeUrinal

PSET_TYPEDRIVENOVERRIDE / IfcSanitaryTerminal / URINAL

Natural language names

| Sanitary Terminal Type Urinal

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC4 Addendum 2
Pset_SanitaryTerminalTypeUrinal |  |  |  |
Color |  |  | DELETED |
NominalLength |  |  | DELETED |
NominalWidth |  |  | DELETED |
NominalDepth |  |  | DELETED |

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

UrinalType

P_ENUMERATEDVALUE / IfcLabel / PEnum_UrinalType

| Urinal Type | Selection of the type of urinal from the enumerated list of types where:- Bowl: Individual wall mounted urinal. Slab: Urinal that consists of a slab or sheet fixed to a wall and down which urinal flows into a floor channel. Stall: Floor mounted urinal that consists of an elliptically shaped sanitary stall fixed to a wall and down which urine flows into a floor channel. Trough: Wall mounted urinal of elongated rectangular shape on plan, that can be used by more than one person at a time.
| 小便器タイプ | 下記のリストより小便器タイプを選択 便器：壁に設置された独立した小便器 床：壁や床の溝へ流れるように固定されている 個室：衛生個室の床や壁に楕円形に設置されたフロア 溝：一人以上の人数が同時に使用できるよう、壁に直角に長く引き伸ばした形

Mounting

P_ENUMERATEDVALUE / IfcLabel / PEnum_SanitaryMounting

| Mounting | Selection of the form of mounting from the enumerated list of mountings where:- BackToWall = A pedestal mounted sanitary terminal that fits flush to the wall at the rear to cover its service connections Pedestal = A floor mounted sanitary terminal that has an integral base CounterTop = A sanitary terminal that is installed into a horizontal surface that is installed into a horizontal surface. Note: When applied to a wash hand basin, the term more normally used is ‘vanity’. See also Wash Hand Basin Type specification. WallHung = A sanitary terminal cantilevered clear of the floor . Note that BackToWall, Pedestal and WallHung are allowable values for a urinal.
| 設置 | 下記の設置方法より選択 ・床置き壁排出：接続口の後部に出水口を合わせること。 ・台：床置きの衛生器具には基礎があること。 ・カウンター：衛生器具の表層が水平に設置されていること。※手洗い台として設置された場合「化粧台」として扱うこと。また、洗面台種類の規格表を参照のこと。 ・壁掛け型：衛生器具は片側固定がされ床から離れていること。 床置き壁排出型・台座と壁掛け型は便器と同等とされます。

SpilloverLevel

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Spillover Level | The level at which water spills out of the object.
| 水位 | 継手からの水位。

Link to this page