Beam varying cardinal points

BACnet MVD

### E.9.1 Beam varying cardinal points

Format | ASCII | Size
--- | --- | ---
XML | File | 12040
STEP | File | 5208

View
Design Transfer View

Entity
IfcBeamStandardCase
IfcBeamType
IfcMaterialProfileSetUsage
IfcMaterialProfileSet

This example illustrates four standard case beams, all with an extruded area solid and axis representation. They have different cardinal points to align the I-Shape profiles with the beam axis. Figure 419 shows the beam solids, Figure 420 shows the beam axes.

Figure 419 — Standard case beams with cardinal points. | Figure 420 — Standard case beams with transparent solids showing the axes.

> NOTE There is no color information within the file, the displayed color and the transparency has been set by the target application as a default.

Link to this page