Pset_SwitchingDeviceTypeContactor

BACnet MVD

#### 7.4.4.70 Pset_SwitchingDeviceTypeContactor

PSET_TYPEDRIVENOVERRIDE / IfcSwitchingDevice / CONTACTOR

Natural language names

| Switching Device Type Contactor

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

ContactorType

P_ENUMERATEDVALUE / IfcLabel / PEnum_ContactorType

| Contactor Type | A list of the available types of contactor from which that required may be selected where: CapacitorSwitching: for switching 3 phase single or multi-step capacitor banks. LowCurrent: requires the use of low resistance contacts. MagneticLatching: enables the contactor to remain in the on position when the coil is no longer energized. MechanicalLatching: requires that the contactor is mechanically retained in the on position. Modular: are totally enclosed and self contained. Reversing: has a double set of contactors that are prewired. Standard: is a generic device that controls the flow of power in a circuit on or off.
| 接触器タイプ | 以下より選択が必要となる、接触器の一覧リスト： コンデンサスイッチ：3つのシングルフェーズまたは複数のコンデンサバンクで切り替える。 低流：低い抵抗接触の使用が必要 マグネット式：コイルのエネルギーが無くなった時に切替をONポジションにして有効にする MechanicalLatching：切替器がONポジションを維持するために機械的な仕組みが必要。 モジュール式：閉鎖されている自働型切替器。 リバース：2つの切替器をワイヤーで接続したもの。 標準：回路で電力潮流をオンまたはオフでコントロールする一般的な装置。

Link to this page