Pset_ProtectiveDeviceTypeEarthLeakageCircuitBreaker

BACnet MVD

#### 7.4.4.63 Pset_ProtectiveDeviceTypeEarthLeakageCircuitBreaker

PSET_TYPEDRIVENOVERRIDE / IfcProtectiveDevice / EARTHLEAKAGECIRCUITBREAKER

Natural language names

| Protective Device Type Earth Leakage Circuit Breaker

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

EarthFailureDeviceType

P_ENUMERATEDVALUE / IfcLabel / PEnum_EarthFailureDeviceType

| Earth Failure Device Type | A list of the available types of circuit breaker from which that required may be selected where: Standard: Device that operates without a time delay. TimeDelayed: Device that operates after a time delay.
| 漏電回路遮断機のタイプ | 以下の中から選択が必要となる場合の遮断機タイプのリスト： スタンダード：遅延無しで動作する機器 遅延：一定時間を経た後で動作する機器

Sensitivity

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Sensitivity | The rated rms value of the vector sum of the instantaneous currents flowing in the main circuits of the device which causes the device to operate under specified conditions. (IEC 61008-1).
| 感度 | 装置のメイン回路を流れる瞬時電流の合計ベクトルの関連する rms 値、特定の条件になると機器が動作するようになる（IEC 61008-1)。

Link to this page