Pset_ControllerTypeMultiPosition

BACnet MVD

#### 7.2.4.35 Pset_ControllerTypeMultiPosition

PSET_TYPEDRIVENOVERRIDE / IfcController / MULTIPOSITION

Natural language names

| Controller Type Multi Position

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

ControlType

P_ENUMERATEDVALUE / IfcLabel / PEnum_ControllerMultiPositionType

| Control Type | The type of signal modification effected and applicable ports: INPUT: Controller element is a dedicated input. OUTPUT: Controller element is a dedicated output. VARIABLE: Controller element is an in-memory variable.

Labels

P_TABLEVALUE / IfcInteger / IfcLabel

| Labels | Table mapping values to labels, where each entry corresponds to an integer within the ValueRange.

Range

P_BOUNDEDVALUE / IfcInteger

| Range | The physical range of values supported by the device.

Value

P_BOUNDEDVALUE / IfcInteger

| Value | The expected range and default value. The LowerLimitValue and UpperLimitValue must fall within the physical Range.

Link to this page