Pset_ProtectiveDeviceTrippingCurve

BACnet MVD

#### 7.4.4.49 Pset_ProtectiveDeviceTrippingCurve

PSET_TYPEDRIVENOVERRIDE / IfcProtectiveDevice

Natural language names

| Protective Device Tripping Curve

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

TrippingCurveType

P_ENUMERATEDVALUE / IfcLabel / PEnum_TrippingCurveType

| Tripping Curve Type | The type of tripping curve that is represented by the property set.
| 動作特性曲線のタイプ | 動作特性曲線のタイプを指定。

TrippingCurve

P_TABLEVALUE / IfcElectricCurrentMeasure / IfcTimeMeasure

| Tripping Curve | A curve that establishes the release time of a tripping unit when a particular prospective current is applied. Note that the tripping curve is defined within a Cartesian coordinate system and this fact must be asserted within the property set: (1) Defining value is the Prospective Current which is a list of minimum 2 and maximum 16 numbers providing the currents in [x In] for points in the current/time log/log coordinate space. The curve is drawn as a straight line between two consecutive points. (2) Defined value is a list of minimum 2 and maximum 16 numbers providing the release_time in [s] for points in the current/time log/log coordinate space. The curve is drawn as a straight line between two consecutive points. Note that a defined interpolation.
| 動作特性曲線 | (1)電流/時間の位置[x In]で示される2～16の想定される電流値を定義する。 (2)定義された値は、電流/時間の位置[ｓ]で示される2～16の想定される放電時間。

Link to this page