Pset_ThermalLoadDesignCriteria

BACnet MVD

#### 6.2.4.28 Pset_ThermalLoadDesignCriteria

PSET_TYPEDRIVENOVERRIDE / IfcSpatialElement

Natural language names

| Thermal Load Design Criteria

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

OccupancyDiversity

P_SINGLEVALUE / IfcPositiveRatioMeasure

| Occupancy Diversity | Diversity factor that may be applied to the number of people in the space.
| 居住者の在室率 | 室内居住者の在室率。

OutsideAirPerPerson

P_SINGLEVALUE / IfcVolumetricFlowRateMeasure

| Outside Air Per Person | Design quantity of outside air to be provided per person in the space.
| １人あたりの外気量 | １人あたりの外気量の設計値。

ReceptacleLoadIntensity

P_SINGLEVALUE / IfcReal

| Receptacle Load Intensity | Average power use intensity of appliances and other non-HVAC equipment in the space per unit area.(PowerMeasure/IfcAreaMeasure).
| 単位面積あたり事務機器の平均電力消費量 | 単位面積あたり事務機器など非空調設備の平均電力消費量。 （PowerMeasure/IfcAreaMeasure）

AppliancePercentLoadToRadiant

P_SINGLEVALUE / IfcPositiveRatioMeasure

| Appliance Percent Load To Radiant | Percent of sensible load to radiant heat.
| 放射熱のうち顕熱分の割合 | 放射熱のうち顕熱分負荷の割合。

LightingLoadIntensity

P_SINGLEVALUE / IfcReal

| Lighting Load Intensity | Average lighting load intensity in the space per unit area (PowerMeasure/IfcAreaMeasure).
| 照明負荷率 | 単位面積あたり照明機器の平均電力消費量。 （PowerMeasure/IfcAreaMeasure）

LightingPercentLoadToReturnAir

P_SINGLEVALUE / IfcPositiveRatioMeasure

| Lighting Percent Load To Return Air | Percent of lighting load to the return air plenum.
| リタン空気への照明機器の放熱率 | 照明機器からリタン空気（天井裏）への放熱率。

Link to this page