Qto_MemberBaseQuantities

BACnet MVD

#### 6.1.5.8 Qto_MemberBaseQuantities

QTO_TYPEDRIVENOVERRIDE / IfcMember

Natural language names

| Member Base Quantities

Quantities

QTO-XML

Name | Type | Description
--- | --- | ---

Length

Q_LENGTH

| Länge | Physikalische Länge des Stabs ohne Berücksichtigung von Abschrägungen, Ausklinkungen, und ähnliches.
| Length | Total nominal length of the member, not taking into account any cut-out's or other processing features.

CrossSectionArea

Q_AREA

| Querschnittsfläche | Querschnittsfläche des Stabs.
| Cross Section Area | Total area of the cross section (or profile) of the member.

OuterSurfaceArea

Q_AREA

| Mantelfläche | Mantelfläche des Stabs, die Querschnittsfläche am Anfang und Ende des Stabs wird nicht berücksichtigt.
| Outer Surface Area | Total area of the extruded surfaces of the member (not taking into account the end cap areas), normally generated as perimeter * length.

GrossSurfaceArea

Q_AREA

| Gesamtoberfläche | Gesamte Oberfläche als Summe von Mantelfläche + (2 x Querschnittsfläche). Es soll nur dann angegeben werden, wenn die Mantelfläche und die Querschnittsfläche nicht separat bestimmt werden können).
| Gross Surface Area | Total area of the member, normally generated as perimeter * length + 2 * cross section area. It is the sum of OuterSurfaceArea + (2 x CrossSectionArea) and shall only be given, if the OuterSurfaceArea and CrossSectionArea cannot be established separately.

NetSurfaceArea

Q_AREA

| Nettooberfläche | Nettooberfläche des Stabs, alle Öffnungen und Aussparungen werden von der Mantelfläche abgezogen.
| Net Surface Area | Net surface area of the member, normally generated as perimeter * length + 2 * cross section area taking into account possible processing features (cut-out's, etc.) or openings and recesses.

GrossVolume

Q_VOLUME

| Bruttovolumen | Volumen des Stabs. Alle Öffnungen und Aussparungen werden übermessen.
| Gross Volume | Total gross volume of the member, not taking into account possible processing features (cut-out's, etc.) or openings and recesses.

NetVolume

Q_VOLUME

| Nettovolumen | Volumen des Stabs. Alle Öffnungen und Aussparungen werden abgezogen.
| Net Volume | Total net volume of the member, taking into account possible processing features (cut-out's, etc.) or openings and recesses.

GrossWeight

Q_WEIGHT

| Bruttogewicht | Gewicht des Stabs. Alle Öffnungen und Aussparungen werden übermessen.
| Gross Weight | Total gross weight of the member without add-on parts, not taking into account possible processing features (cut-out's, etc.) or openings and recesses.

NetWeight

Q_WEIGHT

| Nettogewicht | Gewicht des Stabs. Alle Öffnungen und Aussparungen werden abgezogen.
| Net Weight | Total net weight of the member without add-on parts, taking into account possible processing features (cut-out's, etc.) or openings and recesses.

Link to this page