Pset_SanitaryTerminalTypeToiletPan

BACnet MVD

#### 7.6.4.14 Pset_SanitaryTerminalTypeToiletPan

PSET_TYPEDRIVENOVERRIDE / IfcSanitaryTerminal / TOILETPAN

Natural language names

| Sanitary Terminal Type Toilet Pan

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC4 Addendum 2
Pset_SanitaryTerminalTypeToiletPan |  |  |  |
Color |  |  | DELETED |
NominalLength |  |  | DELETED |
NominalWidth |  |  | DELETED |
NominalDepth |  |  | DELETED |

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

ToiletType

P_ENUMERATEDVALUE / IfcLabel / PEnum_ToiletType

| Toilet Type | Enumeration that defines the types of toilet (water closet) arrangements that may be specified where:- BedPanWasher: Enclosed soil appliance in which bedpans and urinal bottles are emptied and cleansed. Chemical: Portable receptacle or soil appliance that receives and retains excrement in either an integral or a separate container, in which it is chemically treated and from which it has to be emptied periodically. CloseCoupled: Toilet suite in which a flushing cistern is connected directly to the water closet pan. LooseCoupled: Toilet arrangement in which a flushing cistern is connected to the water closet pan through a flushing pipe. SlopHopper: Hopper shaped soil appliance with a flushing rim and outlet similar to those of a toilet pan, into which human excrement is emptied for disposal.
| トイレ種類 | トイレ配置は下記に列挙された仕様となります。 便器洗浄機：便器と小便器が空にされ洗浄される周囲が囲まれた電気機器。 ケミカル：別々の容器で排泄物を受けて、保持し、化学的に扱われる、定期的に空にされる携帯用の容器または土機器。 ｼｽﾀｰﾝ直結型：ｼｽﾀｰﾝがが便器に直接密着して設置されたタイプ ｼｽﾀｰﾝ分離型：ｼｽﾀｰﾝがﾊﾟｲﾌﾟを介して便器につながっているタイプ 汚物流し：ホッパーは土壌器具にデザイされており、汚物が流され空になります。

ToiletPanType

P_ENUMERATEDVALUE / IfcLabel / PEnum_ToiletPanType

| Toilet Pan Type | The property enumeration Pset_ToiletPanTypeEnum defines the types of toilet pan that may be specified within the property set Pset_Toilet:- Siphonic: Toilet pan in which excrement is removed by siphonage induced by the flushing water. Squat: Toilet pan with an elongated bowl installed with its top edge at or near floor level, so that the user has to squat. WashDown: Toilet pan in which excrement is removed by the momentum of the flushing water. WashOut: A washdown toilet pan in which excrement falls first into a shallow water filled bowl.
| 便器タイプ | Pset_SanitaryMountingEnumは下記に列挙された便器タイプとして定義されます。 サイホン式：流水を含むサイホンにより汚物が廃棄される便器 和式：便器が床面か淵の高さと同じに配置された便器。使用者はしゃがまなければならない。 ウォッシュダウン式：勢いよく洗い流すことにより便器をきれいにします 洗浄式便器：まず汚物が落ちその後、便器に水が流れます

PanMounting

P_ENUMERATEDVALUE / IfcLabel / PEnum_SanitaryMounting

| Pan Mounting | The property enumeration Pset_SanitaryMountingEnum defines the forms of mounting or fixing of the sanitary terminal that may be specified within property sets used to define sanitary terminals (WC’s, basins, sinks, etc.) where:- BackToWall: A pedestal mounted sanitary terminal that fits flush to the wall at the rear to cover its service connections. Pedestal: A floor mounted sanitary terminal that has an integral base. CounterTop: A sanitary terminal that is installed into a horizontal surface that is installed into a horizontal surface. Note: When applied to a wash hand basin, the term more normally used is ‘vanity’. See also Wash Hand Basin Type specification. WallHung: A sanitary terminal cantilevered clear of the floor.
| 取付方法 | Pset_SanitaryMountingEnumは固定された衛生器具の接続点（トイレや洗面器、シンクなど）に取り付けられます。 ・床置き壁排出：背面の壁に接続口を合わせること。 ・台：床置きの衛生器具には基礎があること。 ・カウンター：衛生器具の表層が水平に設置されていること。※手洗い台として設置された場合「化粧台」として扱うこと。また、洗面台種類の規格表を参照のこと。 ・壁掛け型：衛生器具は片側固定がされ床から離れていること。

SpilloverLevel

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Spillover Level | The level at which water spills out of the terminal.
| 水位 | 継手からの水位。

Link to this page