Pset_UnitaryControlElementPHistory

BACnet MVD

#### 7.2.4.68 Pset_UnitaryControlElementPHistory

PSET_PERFORMANCEDRIVEN / IfcUnitaryControlElement

Natural language names

| Unitary Control Element PHistory

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

Temperature

P_REFERENCEVALUE / IfcTimeSeries / IfcThermodynamicTemperatureMeasure

| Temperature | Indicates the current measured temperature.

Mode

P_REFERENCEVALUE / IfcTimeSeries / IfcIdentifier

| Mode | Indicates operation mode corresponding to Pset_UnitaryControlTypeCommon.Mode. For example, 'HEAT', 'COOL', 'AUTO'.

Fan

P_REFERENCEVALUE / IfcTimeSeries / IfcLogical

| Fan | Indicates fan operation where True is on, False is off, and Unknown is automatic.

SetPoint

P_REFERENCEVALUE / IfcTimeSeries / IfcIdentifier

| Set Point | Indicates the temperature setpoint. For thermostats with setbacks or separate high and low setpoints, then the time series may contain a pair of values at each entry where the first value is the heating setpoint (low) and the second value is the cooling setpoint (high).

Link to this page