Pset_ProtectiveDeviceTrippingFunctionICurve

BACnet MVD

#### 7.4.4.51 Pset_ProtectiveDeviceTrippingFunctionICurve

PSET_TYPEDRIVENOVERRIDE / IfcProtectiveDeviceTrippingUnit

Natural language names

| Protective Device Tripping Function ICurve

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

IsSelectable

P_SINGLEVALUE / IfcBoolean

| Is Selectable | Indication whether the S-function can be switched off or not.
| 切り替え | 装置の “ON-OFF”状態を電気的表示が切り替え可能かどうか。

NominalCurrentAdjusted

P_SINGLEVALUE / IfcBoolean

| Nominal Current Adjusted | An indication if the tripping currents of the short time protection is related to the nominal current multiplied with the actual setting of the current adjustment, if any, of the long time protection part of the protective device, or not.
| 定格調整電流 | 電流によって、動作時間が短かかったり長かったりするかどうか。

ReleaseCurrent

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Release Current | The release current in [x In] for the initial tripping of the S-function.
| 放出電流 | 放出する電流は、S-functionの初期特性。

ReleaseTime

P_SINGLEVALUE / IfcTimeMeasure

| Release Time | The release time in [s] for the initial tripping of the relevant part. This time indicates that for current lower than the indicated release current, the tripping time will be longer than the indicated release time. The value is given as a mean value.
| 放出時間 | 関連する部分の初期トリップのための[s]が放出時間。 このトリップ時間は、リリースの電流よりも低い電流の場合、指定された動作時間よりも長くなります。 値が平均値として与えられる。

CurrentTolerance1

P_SINGLEVALUE / IfcPositiveRatioMeasure

| Current Tolerance1 | The tolerance for the current of time/current-curve in [%].
| 許容電流1 | 時間/特性曲線の許容範囲を[％]で指定。

CurrentToleranceLimit1

P_SINGLEVALUE / IfcTimeMeasure

| Current Tolerance Limit1 | The time limit in [s] limiting the application of CurrentTolerance1, if any. If the value is set to 0, the value of the CurrentTolerance1 is valid for the whole time/current-curve.
| 許容電流限界1 | 許容電流1を制限する時間制限。 値が0の場合は、制限はない。

CurrentTolerance2

P_SINGLEVALUE / IfcPositiveRatioMeasure

| Current Tolerance2 | The tolerance for the current of time/current-curve in [%] valid for times above CurrentTolereanceLimit1.
| 許容電流2 | [％]で指定された時間/特性曲線の許容範囲は、上記の許容電流限界1の時間で有効です。

IsCurrentTolerancePositiveOnly

P_SINGLEVALUE / IfcBoolean

| Is Current Tolerance Positive Only | Indication whether the value of CurrentTolerance1 is provided as a positive tolereance only or not. If not, the value is proved as a pluss/minus tolerance.
| 電流許容値 | 許容電流限界1の値のみかどうか 上記でない場合、電流許容値はプラス/マイナスした値。

TimeTolerance1

P_SINGLEVALUE / IfcPositiveRatioMeasure

| Time Tolerance1 | The tolerance for the time of time/current-curve in [%].
| 許容時間1 | [％]で時間/特性曲線の許容時間を設定。

TimeToleranceLimit1

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Time Tolerance Limit1 | The current limit in [x In] limiting the application of TimeTolerance1, if any. If the value is set to 0, the value of the TimeTolerance1 is valid for the whole time/current-curve.
| 許容限界時間1 | 許容時間1を制限する電流制限値。 値が0の場合は、制限はない。

TimeTolerance2

P_SINGLEVALUE / IfcPositiveRatioMeasure

| Time Tolerance2 | The tolerance for the time of the time/current-curve in [%] valid for currents above TimeToleranceLimit1.
| 許容時間2 | [％]で指定された時間/特性曲線の許容範囲は、上記の許容電流限界1の電流で有効です。

IsTimeTolerancePositiveOnly

P_SINGLEVALUE / IfcBoolean

| Is Time Tolerance Positive Only | Indication whether the value of TimeTolerance1 is provided as a positive tolereance only or not. If not, the value is proved as a pluss/minus tolerance.
| 時間許容値 | 許容時間1の値のみかどうか 上記でない場合、時間許容値は、プラス/マイナスした値。

MaxAdjustmentX_ICS

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Max Adjustment X_ ICS | Provides the maximum setting value for the available current adjustment in relation to the Ics breaking capacity of the protection device of which the actual tripping unit is a part of. The value is not asserted unless the instantaneous time protection is.
| 最大調整X_ICS | 実際のトリップ装置の一部である保護装置のIcs 遮断容量に関連して利用可能な電流の最大調整値。

IsOffWhenSFunctionOn

P_SINGLEVALUE / IfcBoolean

| Is Off When SFunction On | Indication whether the I-function is automatically switched off when the S-function is switched on.

Link to this page