Pset_ElectricFlowStorageDeviceTypeCommon

BACnet MVD

#### 7.4.4.33 Pset_ElectricFlowStorageDeviceTypeCommon

PSET_TYPEDRIVENOVERRIDE / IfcElectricFlowStorageDevice

Natural language names

| Electric Flow Storage Device Type Common

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

Reference

P_SINGLEVALUE / IfcIdentifier *

| Bauteiltyp | Bezeichnung zur Zusammenfassung gleichartiger Bauteile zu einem Bauteiltyp (auch Konstruktionstyp genannt). Alternativ zum Namen des "Typobjekts", insbesondere wenn die Software keine Typen unterstützt.
| Reference | Reference ID for this specified type in this project (e.g. type 'A-1'), Also referred to as "construction type". It should be provided as an alternative to the name of the "object type", if the software does not support object types.
| Reference | Référence à l'identifiant d'un type spécifié dans le contexte du projet (exemple : "type A1") pour désigner un "type de construction". Une alternative au nom d'un objet type lorsque les objets types ne sont pas gérés par le logiciel.
| 参照記号 | このプロジェクトにおける参照記号(例：A-1)。分類コードではなく内部で使用されるプロジェクトタイプとして使用されるもの。
| 参考号 | 若未采用已知的分类系统，则该属性为该项目中该类型构件的参考编号（例如，类型A-1）。

Status

P_ENUMERATEDVALUE / IfcLabel / PEnum_ElementStatus*

| Status | Status bzw. Phase des Bauteils insbesondere beim Bauen im Bestand. "Neu" (new) neues Bauteil als Ergänzung, "Bestand" (existing) bestehendes Bauteil, dass erhalten bleibt, "Abbruch" (demolish) Bauteil, das abgebrochen wird, "Temporär" (temporary) Bauteil und andere Bauelemente, die vorübergehend eingebaut werden (wie Abstützungen, etc.)
| Status | Status of the element, predominately used in renovation or retrofitting projects. The status can be assigned to as "New" - element designed as new addition, "Existing" - element exists and remains, "Demolish" - element existed but is to be demolished, "Temporary" - element will exists only temporary (like a temporary support structure).
| Statut | Statut de l'élément, principalement utilisé dans les projets de rénovation et de réhabilitation. Le statut a pour valeur NOUVEAU pour un nouvel élément, EXISTANT pour un élément existant qui est conservé, DEMOLI pour un élément existant à démolir et TEMPORAIRE pour un élément temporaire (comme une structure support provisoire).
| 状態 | 要素（主にリノベーションまたは改修プロジェクトにおいて）の状態。 状態は、「新規(New)」－新しく追加される要素。「既存」－要素は存在し、かつ残りもの。「破壊」－要素は存在したが、廃棄されるもの。「一時的」－一時的に存在する要素（一時的にサポートしている構造のようなもの）。

NominalSupplyVoltage

P_SINGLEVALUE / IfcElectricVoltageMeasure

| Nominal Supply Voltage | The nominal voltage of the supply.
| 公称電圧 | 電源の公称電圧。

NominalSupplyVoltageOffset

P_BOUNDEDVALUE / IfcElectricVoltageMeasure

| Nominal Supply Voltage Offset | The maximum and minimum allowed voltage of the supply e.g. boundaries of 380V/440V may be applied for a nominal voltage of 400V.
| オフセット公称電圧 | 電源の最大値と最小許容電圧。たとえば380V/440Vの境界は400Vの公称電圧に適用される。

NominalFrequency

P_SINGLEVALUE / IfcFrequencyMeasure

| Nominal Frequency | The nominal frequency of the supply.
| 公称周波数 | 電源の公称周波数。

ConnectedConductorFunction

P_ENUMERATEDVALUE / IfcLabel / PEnum_ConductorFunctionEnum

| Connected Conductor Function | Function of the conductors to which the load is connected.
| 接続導体機能 | 導体の機能は負荷が接続された状態。

ShortCircuit3PoleMaximumState

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Short Circuit3 Pole Maximum State | Maximum 3 pole short circuit current provided at the point of supply.
| 3極最大短絡電流 | 電源供給時点の3極最大短絡電流。

ShortCircuit3PolePowerFactorMaximumState

P_SINGLEVALUE / IfcReal

| Short Circuit3 Pole Power Factor Maximum State | Power factor of the maximum 3 pole short circuit current provided at the point of supply.
| 3極最大短絡電流力率 | 電源供給時点の3極最大短絡電流力率。

ShortCircuit2PoleMinimumState

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Short Circuit2 Pole Minimum State | Minimum 2 pole short circuit current provided at the point of supply.
| 2極最小短絡電流 | 電源供給時点の2極最小短絡電流。

ShortCircuit2PolePowerFactorMinimumState

P_SINGLEVALUE / IfcReal

| Short Circuit2 Pole Power Factor Minimum State | Power factor of the minimum 2 pole short circuit current provided at the point of supply.
| 2極最小短絡電流力率 | 電源供給時点の2極最小短絡電流力率。

ShortCircuit1PoleMaximumState

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Short Circuit1 Pole Maximum State | Maximum 1 pole short circuit current provided at the point of supply i.e. the fault between 1 phase and N.
| 1極最大短絡電流 | 電源供給時点の点1相とN間の1極最大短絡電流。

ShortCircuit1PolePowerFactorMaximumState

P_SINGLEVALUE / IfcReal

| Short Circuit1 Pole Power Factor Maximum State | Power factor of the maximum 1 pole short circuit current provided at the point of supply i.e. the fault between 1 phase and N.
| 1極最大短絡電流力率 | 電源供給時点の点1相とN間の1極最大短絡電流力率。

ShortCircuit1PoleMinimumState

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Short Circuit1 Pole Minimum State | Minimum 1 pole short circuit current provided at the point of supply i.e. the fault between 1 phase and N.
| 1極最小短絡電流 | 電源供給時点の点1相とN間の1極最小短絡電流。

ShortCircuit1PolePowerFactorMinimumState

P_SINGLEVALUE / IfcReal

| Short Circuit1 Pole Power Factor Minimum State | Power factor of the minimum 1 pole short circuit current provided at the point of supply i.e. the fault between 1 phase and N.
| 1極最小短絡電流力率 | 電源供給時点の点1相とN間の1極最小短絡電流力率。

EarthFault1PoleMaximumState

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Earth Fault1 Pole Maximum State | Maximum 1 pole earth fault current provided at the point of supply i.e. the fault between 1 phase and PE/PEN.
| 1極最大地絡電流 | 電源供給時点の点1相とPE/PEN間の1極最大地絡電流。

EarthFault1PolePowerFactorMaximumState

P_SINGLEVALUE / IfcReal

| Earth Fault1 Pole Power Factor Maximum State | Power factor of the maximum 1 pole earth fault current provided at the point of supply i.e. the fault between 1 phase and PE/PEN.
| 1極最大地絡電流力率 | 電源供給時点の点1相とPE/PEN間の1極最大地絡電流力率。

EarthFault1PoleMinimumState

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Earth Fault1 Pole Minimum State | Minimum 1 pole earth fault current provided at the point of supply i.e. the fault between 1 phase and PE/PEN.
| 1極最小地絡電流 | 電源供給時点の点1相とPE/PEN間の1極最小地絡電流。

EarthFault1PolePowerFactorMinimumState

P_SINGLEVALUE / IfcReal

| Earth Fault1 Pole Power Factor Minimum State | Power factor of the minimum 1 pole earth fault current provided at the point of supply i.e. the fault between 1 phase and PE/PEN.
| 1極最小地絡電流力率 | 電源供給時点の点1相とPE/PEN間の1極最小地絡電流力率。

Link to this page