Pset_ProtectiveDeviceTrippingUnitCurrentAdjustment

BACnet MVD

#### 7.4.4.54 Pset_ProtectiveDeviceTrippingUnitCurrentAdjustment

PSET_TYPEDRIVENOVERRIDE / IfcProtectiveDeviceTrippingUnit

Natural language names

| Protective Device Tripping Unit Current Adjustment

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

AdjustmentValueType

P_ENUMERATEDVALUE / IfcLabel / PEnum_AdjustmentValueType

| Adjustment Value Type | The type of adjustment value that is applied through the property set. This determines the properties that should be asserted (see below).
| 調整値の型 | 調整値のタイプを設定。

AdjustmentRange

P_BOUNDEDVALUE / IfcElectricCurrentMeasure

| Adjustment Range | Upper and lower current adjustment limits for an AdjustmentValueType = RANGE. Note that this property should not have a value for an AdjustmentValueType = LIST.
| 調整範囲 | 時間調整の範囲の上限値と下限値を設定。一覧表ではもっていない事を注意。

AdjustmentRangeStepValue

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Adjustment Range Step Value | Step value of current adjustment for an AdjustmentValueType = RANGE. Note that this property should not have a value for an AdjustmentValueType = LIST.
| 調整範囲のステップ値 | 時間調整の範囲をステップ値を設定。一覧表ではもっていない事を注意。

AdjustmentValues

P_LISTVALUE / IfcElectricCurrentMeasure

| Adjustment Values | A list of current adjustment values that may be applied to a tripping unit for an AdjustmentValueType = LIST. A minimum of 1 and a maximum of 16 adjustment values may be specified. Note that this property should not have a value for an AdjustmentValueType = RANGE.
| 調整値 | 時間調整値を１から16で設定。範囲では、ない事を注意。

AdjustmentDesignation

P_SINGLEVALUE / IfcLabel

| Adjustment Designation | The desgnation on the device for the adjustment.
| 調整の指定 | 調整する装置の指定。

Link to this page