Pset_ProtectiveDeviceBreakerUnitI2TFuseCurve

BACnet MVD

#### 7.4.4.44 Pset_ProtectiveDeviceBreakerUnitI2TFuseCurve

PSET_TYPEDRIVENOVERRIDE / IfcProtectiveDevice

Natural language names

| Protective Device Breaker Unit I2 TFuse Curve

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

VoltageLevel

P_ENUMERATEDVALUE / IfcLabel / PEnum_VoltageLevels

| Voltage Level | The voltage levels of the fuse for which the data of the instance is valid. More than one value may be selected in the enumeration.
| 電圧レベル | 電圧レベルを選択。

BreakerUnitFuseMeltingCurve

P_TABLEVALUE / IfcElectricCurrentMeasure / IfcReal

| Breaker Unit Fuse Melting Curve | A curve that establishes the energy required to melt the fuse of a breaker unit when a particular prospective melting current is applied. Note that the breaker unit fuse melting curve is defined within a Cartesian coordinate system and this fact must be: (1) Defining value: ProspectiveCurrentMelting :A list of minimum 2 and maximum 8 numbers providing the currents in [A] for points in the current/melting_energy log/log coordinate space. The curve is drawn as a straight line between two consecutive points. (2) Defined value: MeltingEnergy: A list of minimum 2 and maximum 8 numbers providing the energy whereby the fuse is starting to melt, I2t, in [A2s] for points in the current/melting_energy log/log coordinate space. The curve is drawn as a straight line between two consecutive points.
| フューズ遮断機融解曲線 | 想定外の電流が流れた時に遮断機のフューズを溶かすために必要なエネルギーを表す曲線。 想定外の電流が流れた時に遮断機のフューズを溶かすために必要なエネルギーを表す曲線。 （1）定義値：融解電流：電流/ 融解エネルギーで示される最小2から最大8のリストで電流[A]を定義します。 カーブが連続する2つの点を結ぶ直線として描かれています。 （2）定義値：融解エネルギー：/電流/融解エネルギーの位置[A2s]で示される2～16の想定されるフューズが溶解始める電流[A2s]を定義します。カーブが連続する2つの点を結ぶ直線として描かれています。

BreakerUnitFuseBreakingingCurve

P_TABLEVALUE / IfcElectricCurrentMeasure / IfcReal

| Breaker Unit Fuse Breakinging Curve | A curve that establishes the let through breaking energy of a breaker unit when a particular prospective breaking current is applied. Note that the breaker unit fuse breaking curve is defined within a Cartesian coordinate system and this fact must be: (1) Defining value: ProspectiveCurrentBreaking: A list of minimum 2 and maximum 8 numbers providing the currents in [A] for points in the current/breaking energy log/log coordinate space. The curve is drawn as a straight line between two consecutive points. (2) Defined value: LetThroughBreakingEnergy: A list of minimum 2 and maximum 8 numbers providing the breaking energy whereby the fuse has provided a break, I2t, in [A2s] for points in the current/breakting_energy log/log coordinate space. The curve is drawn as a straight line between two consecutive.
| フューズ遮断機融解曲線 | 想定外の電流が流れた時に遮断機のフューズを溶かすために必要なエネルギーを表す曲線。 想定外の電流が流れた時に遮断機のフューズを溶かすために必要なエネルギーを表す曲線。 （1）定義値：融解電流：電流/ 融解エネルギーで示される最小2から最大8のリストで電流[A]を定義します。 カーブが連続する2つの点を結ぶ直線として描かれています。 （2）定義値：融解エネルギー：/電流/融解エネルギーの位置[A2s]で示される2～16の想定されるフューズが溶解始める電流[A2s]を定義します。カーブが連続する2つの点を結ぶ直線として描かれています。

Link to this page