Pset_PipeFittingTypeJunction

BACnet MVD

#### 7.5.4.74 Pset_PipeFittingTypeJunction

PSET_TYPEDRIVENOVERRIDE / IfcPipeFitting / JUNCTION

Natural language names

| Pipe Fitting Type Junction

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

JunctionType

P_ENUMERATEDVALUE / IfcLabel / PEnum_PipeFittingJunctionType

| Junction Type | The type of junction. TEE=3 ports, CROSS = 4 ports.
| 継ぎ手タイプ | 接合のタイプ　(T継ぎ手は3本　十字継ぎ手は4本)

JunctionLeftAngle

P_SINGLEVALUE / IfcPositivePlaneAngleMeasure

| Junction Left Angle | The change of direction of flow for the left junction.
| 左継ぎ手角度 | 左継ぎ手の流れの方向の変化

JunctionLeftRadius

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Junction Left Radius | The radius of bending for the left junction.
| 左継ぎ手半径 | 左継ぎ手の曲がりの半径

JunctionRightAngle

P_SINGLEVALUE / IfcPositivePlaneAngleMeasure

| Junction Right Angle | The change of direction of flow for the right junction where 0 indicates straight segment.
| 右継ぎ手角度 | 右継ぎ手の流れの方向の変化

JunctionRightRadius

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Junction Right Radius | The radius of bending for the right junction where 0 indicates sharp bend.
| 右継ぎ手半径 | 右継ぎ手の曲がりの半径(ゼロは鋭い曲がりを意味する)

Link to this page