Pset_CableSegmentTypeCableSegment

BACnet MVD

#### 7.4.4.20 Pset_CableSegmentTypeCableSegment

PSET_TYPEDRIVENOVERRIDE / IfcCableSegment / CABLESEGMENT

Natural language names

| Cable Segment Type Cable Segment

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

Standard

P_SINGLEVALUE / IfcLabel

| Standard | The designation of the standard applicable for the definition of the Cable/Bus used.
| 標準 | 使用されるケーブル、busbarの定義のために使用される標準仕様。

NumberOfCores

P_SINGLEVALUE / IfcInteger

| Number Of Cores | The number of cores in Cable/Bus.
| 芯数 | ケーブルや母線の芯数を示す。

OverallDiameter

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Overall Diameter | The overall diameter of a Cable/Bus.
| 直径 | ケーブルや母線の外形寸法（直径）を示す。

RatedVoltage

P_BOUNDEDVALUE / IfcElectricVoltageMeasure *

| Rated Voltage | The voltage that a device is designed to handle.

RatedTemperature

P_BOUNDEDVALUE / IfcThermodynamicTemperatureMeasure

| Rated Temperature | The range of allowed temerature that a device is certified to handle. The upper bound of this value is the maximum.
| 定格温度 | 使用できることが許可されている許容温度。

ScreenDiameter

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Screen Diameter | The diameter of the screen around a cable or bus segment (if present).
| スクリーン径 | 遮へい層の径、厚さ。

HasProtectiveEarth

P_SINGLEVALUE / IfcBoolean *

| Has Protective Earth | Indicates whether the electrical device has a protective earth connection (=TRUE) or not (= FALSE).

MaximumOperatingTemperature

P_SINGLEVALUE / IfcThermodynamicTemperatureMeasure

| Maximum Operating Temperature | The maximum temperature at which a cable or bus is certified to operate.
| 許容最高温度 | ケーブルや母線の最大動作温度を示す。

MaximumShortCircuitTemperature

P_SINGLEVALUE / IfcThermodynamicTemperatureMeasure

| Maximum Short Circuit Temperature | The maximum short circuit temperature at which a cable or bus is certified to operate.
| 短絡許容最高温度 | ケーブルや母線の最大短絡温度を示す。

SpecialConstruction

P_SINGLEVALUE / IfcLabel

| Special Construction | Special construction capabilities like self-supporting, flat devidable cable or bus flat non devidable cable or bus supporting elements inside (steal, textile, concentric conductor). Note that materials used should be agreed between exchange participants before use.
| 特別な施工方法 | 特殊な構造を備えた性能－たとえば、平型フレキシブルケーブルあるいは硬い平型母線ケーブル、あるいは母線で内部に鉄製、繊維、同心導体で構成されているサポートを持っている。 注記）使用する材料は、使用前に交流参加者間で合意すること。

Weight

P_SINGLEVALUE / IfcMassMeasure

| Weight | Weight of cable kg/km.
| 重量 | ケーブルの重量。

SelfExtinguishing60332_1

P_SINGLEVALUE / IfcBoolean

| Self Extinguishing60332_1 | Self Extinguishing cable/core according to IEC 60332.1.
| 自己消火ケーブル | IEC 60332.1.に規定されている自己消火ケーブル。

SelfExtinguishing60332_3

P_SINGLEVALUE / IfcBoolean

| Self Extinguishing60332_3 | Self Extinguishing cable/core according to IEC 60332.3.
| 自己消火ケーブル | IEC 60332.3.に規定されている自己消火ケーブル。

HalogenProof

P_SINGLEVALUE / IfcBoolean

| Halogen Proof | Produces small amount of smoke and irritating Deaerator/Gas.
| エコケーブル | 煙や刺激臭のあるガスの発生が少ないケーブル。

FunctionReliable

P_SINGLEVALUE / IfcBoolean

| Function Reliable | Cable/bus maintain given properties/functions over a given (tested) time and conditions. According to IEC standard.
| 信頼性のある機能 | ケーブルや母線が与えられた時間と条件の中で規定される機能、性質を維持すること。これはIEC基準による。

Link to this page