Pset_CooledBeamTypeActive

BACnet MVD

#### 7.5.4.25 Pset_CooledBeamTypeActive

PSET_TYPEDRIVENOVERRIDE / IfcCooledBeam / ACTIVE

Natural language names

| Cooled Beam Type Active

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

AirFlowConfiguration

P_ENUMERATEDVALUE / IfcLabel / PEnum_CooledBeamActiveAirFlowConfigurationType

| Air Flow Configuration | Air flow configuration type of cooled beam.

AirflowRateRange

P_BOUNDEDVALUE / IfcVolumetricFlowRateMeasure

| Airflow Rate Range | Possible range of airflow that can be delivered.

SupplyAirConnectionType

P_ENUMERATEDVALUE / IfcLabel / PEnum_CooledBeamSupplyAirConnectionType

| Supply Air Connection Type | The manner in which the pipe connection is made to the cooled beam.

ConnectionSize

P_SINGLEVALUE / IfcLengthMeasure

| Connection Size | Duct connection diameter.

Link to this page