Pset_ProtectiveDeviceBreakerUnitI2TCurve

BACnet MVD

#### 7.4.4.43 Pset_ProtectiveDeviceBreakerUnitI2TCurve

PSET_TYPEDRIVENOVERRIDE / IfcProtectiveDevice

Natural language names

| Protective Device Breaker Unit I2 TCurve

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

VoltageLevel

P_ENUMERATEDVALUE / IfcLabel / PEnum_VoltageLevels

| Voltage Level | The voltage levels of the protective device for which the data of the instance is valid. More than one value may be selected in the enumeration.
| 電圧レベル | 保護装置が作動する電圧レベルを選択。 [U230,U400,U525,U690,U1000,その他,不明,無]

NominalCurrent

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Nominal Current | A set of nominal currents in [A] for which the data of this instance is valid. At least one value shall be provided. Any value in the set shall not exceed the value of the UltimateRatedCurrent associated with the same breaker unit.
| 定格電流 | 定格電流[A]を少なくても1つ値をセットしなければならない。 セット内の任意の値の値を超えてはならない。 定格電流は、同じブレーカ部に関連付けられている。

BreakerUnitCurve

P_TABLEVALUE / IfcElectricCurrentMeasure / IfcReal

| Breaker Unit Curve | A curve that establishes the let through energy of a breaker unit when a particular prospective current is applied. Note that the breaker unit curve is defined within a Cartesian coordinate system and this fact must be asserted within the property set: (1) Defining value: ProspectiveCurrent: A list of minimum 2 and maximum 16 numbers providing the currents in [A] for points in the current/I2t log/log coordinate space. The curve is drawn as a straight line between two consecutive points. (2) Defined value: LetThroughEnergy: A list of minimum 2 and maximum 16 numbers providing the let-through energy, I2t, in [A2s] for points in the current/I2t log/log coordinate space. The curve is drawn as a straight line between two consecutive points.
| 遮断機曲線 | 適用された電流と通過する遮断機のエネルギーを示した曲線 （1）定義値：ProspectiveCurrent（固有電流）： 電流/I2tで示される最小2から最大8のリストで電流[A]を定義します。 カーブが連続する2つの点を結ぶ直線として描かれています。 （2）定義値：LetThroughEnergy： 電流/I2tで示される最小2から最大8のリストで通過エネルギー電流[[A2s]を定義します。 カーブが連続する2つの点を結ぶ直線として描かれています。

Link to this page