Pset_ElectricalDeviceCommon

BACnet MVD

#### 7.4.4.26 Pset_ElectricalDeviceCommon

PSET_TYPEDRIVENOVERRIDE / IfcDistributionElement

Natural language names

| Electrical Device Common

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC4 Addendum 2
Pset_ElectricalDeviceCommon |  |  |  |
IK_Code |  |  | ADDED |

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

RatedCurrent

P_BOUNDEDVALUE / IfcElectricCurrentMeasure

| Rated Current | The current that a device is designed to handle.

RatedVoltage

P_BOUNDEDVALUE / IfcElectricVoltageMeasure

| Rated Voltage | The voltage that a device is designed to handle.

NominalFrequencyRange

P_BOUNDEDVALUE / IfcFrequencyMeasure

| Nominal Frequency Range | The upper and lower limits of frequency for which the operation of the device is certified.

PowerFactor

P_SINGLEVALUE / IfcNormalisedRatioMeasure

| Power Factor | The ratio between the rated electrical power and the product of the rated current and rated voltage

ConductorFunction

P_ENUMERATEDVALUE / IfcLabel / PEnum_ConductorFunctionEnum

| Conductor Function | Function of a line conductor to which a device is intended to be connected where L1, L2 and L3 represent the phase lines according to IEC 60446 notation (sometimes phase lines may be referenced by color [Red, Blue, Yellow] or by number [1, 2, 3] etc). Protective Earth is sometimes also known as CPC or common protective conductor. Note that for an electrical device, a set of line conductor functions may be applied.

NumberOfPoles

P_SINGLEVALUE / IfcInteger

| Number Of Poles | The number of live lines that is intended to be handled by the device.

HasProtectiveEarth

P_SINGLEVALUE / IfcBoolean

| Has Protective Earth | Indicates whether the electrical device has a protective earth connection (=TRUE) or not (= FALSE).

InsulationStandardClass

P_ENUMERATEDVALUE / IfcLabel / PEnum_InsulationStandardClass

| Insulation Standard Class | Insulation standard classes provides basic protection information against electric shock. Defines levels of insulation required in terms of constructional requirements (creepage and clearance distances) and electrical requirements (compliance with electric strength tests). Basic insulation is considered to be shorted under single fault conditions. The actual values required depend on the working voltage to which the insulation is subjected, as well as other factors. Also indicates whether the electrical device has a protective earth connection.

IP_Code

P_SINGLEVALUE / IfcLabel

| IP_ Code | IP Code, the International Protection Marking, IEC 60529), classifies and rates the degree of protection provided against intrusion.

IK_Code

P_SINGLEVALUE / IfcLabel

IK Code according to IEC 62262 (2002) is a numeric classification for the degree of protection provided by enclosures for electrical equipment against external mechanical impacts.

> NOTE In earlier labeling, the third numeral (1..) had been occasionally added to the closely related IP Code on ingress protection, to indicate the level of impact protection.

Link to this page