Pset_ProtectiveDeviceOccurrence

BACnet MVD

#### 7.4.4.48 Pset_ProtectiveDeviceOccurrence

PSET_OCCURRENCEDRIVEN / IfcProtectiveDevice

Natural language names

| Protective Device Occurrence

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

PoleUsage

P_ENUMERATEDVALUE / IfcLabel / PEnum_PoleUsage

| Pole Usage | Pole usage.

LongTimeFunction

P_SINGLEVALUE / IfcBoolean

| Long Time Function | Applying long time function A flag indicating that the long time function (i.e. the thermal tripping) of the device is used. The value should be set to TRUE for all devices except those that allows the Long time function of the device not to be used.

ShortTimeFunction

P_SINGLEVALUE / IfcBoolean

| Short Time Function | Applying short time function A flag indicating that the short time function of the device is used. The value should be set to FALSE for devices not having a short time function, or if the short time function is not selected to be used.

ShortTimei2tFunction

P_SINGLEVALUE / IfcBoolean

| Short Timei2t Function | Applying short time i2t function. A flag indicating that the I2t short time function of the device is used. The value should be set to TRUE only if the I2t function is explicitly selected for the device.

GroundFaultFunction

P_SINGLEVALUE / IfcBoolean

| Ground Fault Function | Applying ground fault function. A flag indicating that the ground fault function of the device is used. The value should be set to FALSE for devices not having a ground fault function, or if the ground fault function is not selected to be used.

GroundFaulti2tFunction

P_SINGLEVALUE / IfcBoolean

| Ground Faulti2t Function | Applying ground fault i2t function. A flag indicating that the I2t ground fault function of the device is used. The value should be set to TRUE only if the I2t function is explicitly selected for the device.

LongTimeCurrentSetValue

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Long Time Current Set Value | Long time current set value. The set value of the long time tripping current if adjustable.

ShortTimeCurrentSetValue

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Short Time Current Set Value | Short time current set value. The set value of the long time tripping current if adjustable.

InstantaneousCurrentSetValue

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Instantaneous Current Set Value | Instantaneous current set value. The set value of the instantaneous tripping current if adjustable.

GroundFaultCurrentSetValue

P_SINGLEVALUE / IfcElectricCurrentMeasure

| Ground Fault Current Set Value | Ground fault current set value. The set value of the ground tripping current if adjustable.

LongTimeDelay

P_SINGLEVALUE / IfcTimeMeasure

| Long Time Delay | Long time delay. The set value of the long time time-delay if adjustable.

ShortTimeTrippingTime

P_SINGLEVALUE / IfcTimeMeasure

| Short Time Tripping Time | Short time tripping time. The set value of the short time tripping time if adjustable.

InstantaneousTrippingTime

P_SINGLEVALUE / IfcTimeMeasure

| Instantaneous Tripping Time | Instantaneous tripping time. The set value of the instantaneous tripping time if adjustable.

GroundFaultTrippingTime

P_SINGLEVALUE / IfcTimeMeasure

| Ground Fault Tripping Time | Ground fault tripping time. The set value of the ground fault tripping current if adjustable.

Link to this page