Pset_UnitaryEquipmentTypeAirConditioningUnit

BACnet MVD

#### 7.5.4.97 Pset_UnitaryEquipmentTypeAirConditioningUnit

PSET_TYPEDRIVENOVERRIDE / IfcUnitaryEquipment / AIRCONDITIONINGUNIT

Natural language names

| Unitary Equipment Type Air Conditioning Unit

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

SensibleCoolingCapacity

P_SINGLEVALUE / IfcPowerMeasure

| Sensible Cooling Capacity | Sensible cooling capacity.
| 顕熱冷却能力 | 顕熱冷却能力

LatentCoolingCapacity

P_SINGLEVALUE / IfcPowerMeasure

| Latent Cooling Capacity | Latent cooling capacity.
| 潜熱冷却能力 | 潜熱冷却能力

CoolingEfficiency

P_SINGLEVALUE / IfcPositiveRatioMeasure

| Cooling Efficiency | Coefficient of Performance: Ratio of cooling energy output to energy input under full load operating conditions.
| 冷却効率 | 性能係数全負荷運転状態でのエネルギー入力に対する冷却エネルギー出力の割合

HeatingCapacity

P_SINGLEVALUE / IfcPowerMeasure

| Heating Capacity | Heating capacity.
| 加熱容量 | 加熱容量

HeatingEfficiency

P_SINGLEVALUE / IfcPositiveRatioMeasure

| Heating Efficiency | Heating efficiency under full load heating conditions.
| 加熱効率 | 全負荷加熱状態での熱効率

CondenserFlowrate

P_SINGLEVALUE / IfcVolumetricFlowRateMeasure

| Condenser Flowrate | Flow rate of fluid through the condenser.
| 凝縮器流量 | 凝縮器を通る流体の流量

CondenserEnteringTemperature

P_SINGLEVALUE / IfcThermodynamicTemperatureMeasure

| Condenser Entering Temperature | Temperature of fluid entering condenser.
| 凝縮器入口温度 | 凝縮器入口流体温度

CondenserLeavingTemperature

P_SINGLEVALUE / IfcThermodynamicTemperatureMeasure

| Condenser Leaving Temperature | Termperature of fluid leaving condenser.
| 凝縮器出口温度 | 凝縮器出口流体温度

OutsideAirFlowrate

P_SINGLEVALUE / IfcVolumetricFlowRateMeasure

| Outside Air Flowrate | Flow rate of outside air entering the unit.
| 外気流量 | ユニットに入る外気流量

Link to this page