Pset_DistributionChamberElementTypeInspectionChamber

BACnet MVD

#### 6.2.4.4 Pset_DistributionChamberElementTypeInspectionChamber

PSET_TYPEDRIVENOVERRIDE / IfcDistributionChamberElement / INSPECTIONCHAMBER

Natural language names

| Distribution Chamber Element Type Inspection Chamber

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

ChamberLengthOrRadius

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Chamber Length Or Radius | Length or, in the event of the shape being circular in plan, the radius of the chamber.
| チャンバー（バイブスペース？）の長さあるいは半径 | チャンバーの長さあるいは円形チャンバーの半径。

ChamberWidth

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Chamber Width | Width, in the event of the shape being non circular in plan.
| チャンバー（バイブスペース？）の幅 | 非円形チャンバーの幅。

InvertLevel

P_SINGLEVALUE / IfcLengthMeasure

| Invert Level | Level of the lowest part of the cross section as measured from ground level.
| 最大深さ | 断面の最も低い部分の深さ（地面から）。

SoffitLevel

P_SINGLEVALUE / IfcLengthMeasure

| Soffit Level | Level of the highest internal part of the cross section as measured from ground level.
| 最小深さ | 断面の最も高い部分の深さ（地面から）。

WallMaterial

P_REFERENCEVALUE / IfcMaterialDefinition

| Wall Material | The material from which the wall of the chamber is constructed. NOTE: It is assumed that chamber walls will be constructed of a single material.
| 壁の材質 | ダクトスペース壁の材質。 注：ダクトスペースの壁は単層と仮定する

WallThickness

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Wall Thickness | The thickness of the chamber wall construction NOTE: It is assumed that chamber walls will be constructed at a single thickness.
| 壁厚さ | ダクトスペース壁の厚さ。 注：ダクトスペースの壁は単層と仮定する

BaseMaterial

P_REFERENCEVALUE / IfcMaterialDefinition

| Base Material | The material from which the base of the chamber is constructed. NOTE: It is assumed that chamber base will be constructed of a single material.
| 床の材質 | ダクトスペース床面の材質。 注：ダクトスペースの床は単層と仮定する

BaseThickness

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Base Thickness | The thickness of the chamber base construction NOTE: It is assumed that chamber base will be constructed at a single thickness.
| 床の厚さ | ダクトスペース床面の厚さ。 注：ダクトスペースの床は単層と仮定する

WithBackdrop

P_SINGLEVALUE / IfcBoolean

| With Backdrop | Indicates whether the chamber has a backdrop or tumbling bay (TRUE) or not (FALSE).
| バックドロップ付け | ダクトスペースはバックドロップ或いは堰付けかどうか（TRUE或いはFALSE）。

AccessCoverMaterial

P_REFERENCEVALUE / IfcMaterialDefinition

| Access Cover Material | The material from which the access cover to the chamber is constructed. NOTE: It is assumed that chamber walls will be constructed of a single material.
| アクセス（点検）カバーの材質 | アクセス（点検）カバーの材質。 注：バイブスペースの壁は単層と仮定する

AccessLengthOrRadius

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Access Length Or Radius | The length of the chamber access cover or, where the plan shape of the cover is circular, the radius.
| アクセス（点検）カバーの長さ或いは半径 | アクセス（点検）カバーの長さ、或いは円形カバーの半径。

AccessWidth

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Access Width | The width of the chamber access cover where the plan shape of the cover is not circular.
| アクセス（点検）カバーの幅 | アクセス（点検）カバーの幅。

AccessCoverLoadRating

P_SINGLEVALUE / IfcText

| Access Cover Load Rating | The load rating of the access cover (which may be a value or an alphanumerically defined class rating).
| アクセス（点検）カバーの耐荷重 | アクセス（点検）カバーの耐荷重（数字或いはアルファベットで定義する）。

Link to this page