Pset_ProtectiveDeviceTrippingUnitTypeElectronic

BACnet MVD

#### 7.4.4.58 Pset_ProtectiveDeviceTrippingUnitTypeElectronic

PSET_TYPEDRIVENOVERRIDE / IfcProtectiveDeviceTrippingUnit / ELECTRONIC

Natural language names

| Protective Device Tripping Unit Type Electronic

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

ElectronicTrippingUnitType

P_ENUMERATEDVALUE / IfcLabel / PEnum_ElectronicTrippingUnitType

| Electronic Tripping Unit Type | A list of the available types of electronic tripping unit from which that required may be selected.
| 電磁式の装置タイプ | 電磁式の装置タイプをリストから選択。

NominalCurrents

P_LISTVALUE / IfcElectricCurrentMeasure

| Nominal Currents | A set of values providing information on available modules (chips) for setting the nominal current of the protective device. If the set is empty, no nominal current modules are available for the tripping unit.
| 定格電流 | トリップ装置が対応する定格電流。

N_Protection

P_SINGLEVALUE / IfcBoolean

| N_ Protection | An indication whether the electronic tripping unit has separate protection for the N conductor, or not.
| N_Protection | 電磁式トリップ装置がN個の導体を保護するか否かの設定。

N_Protection_50

P_SINGLEVALUE / IfcBoolean

| N_ Protection_50 | An indication whether the electronic tripping unit is tripping if the current in the N conductor is more than 50% of that of the phase conductors. The property is only asserted if the property N_Protection is asserted.
| N_Protection_50 | 電磁式トリップ装置がN導体の50％以上で保護するか否かの設定。

N_Protection_100

P_SINGLEVALUE / IfcBoolean

| N_ Protection_100 | An indication whether the electronic tripping unit is tripping if the current in the N conductor is more than 100% of that of the phase conductors. The property is only asserted if the property N_Protection is asserted.
| N_Protection_100 | 電磁式トリップ装置がN導体の100％以上で保護するか否かの設定。

N_Protection_Select

P_SINGLEVALUE / IfcBoolean

| N_ Protection_ Select | An indication whether the use of the N_Protection can be selected by the user or not. If both the properties N_Protection_50 and N_Protection_100 are asserted, the value of N_Protection_Select property is set to TRUE. The property is only asserted if the property N_Protection is asserted.
| N_Protectionの選択 | どのN_Protectionを使うかユーザが設定できるかどうかを指定する。 N_Protection_50とN_Protection_100の両方が有効な場合は、TRUEにします。

Link to this page