Qto_FootingBaseQuantities

BACnet MVD

#### 7.8.5.1 Qto_FootingBaseQuantities

QTO_TYPEDRIVENOVERRIDE / IfcFooting

Natural language names

| Footing Base Quantities

Quantities

QTO-XML

Name | Type | Description
--- | --- | ---

Length

Q_LENGTH

| Länge | Gesamte Länge des Fundaments, bei Streifenfundamenten entlang der Mittellinie. Sonst eine der beiden horizontalen Abmessungen. Der Wert wird nur angegeben, wenn die Länge konstant ist.
| Length | Length of the footing, not taking into account any cut-out's or other processing features. For strip footings it is measured along the path, for other footings it is one of the horizontal dimensions. It should only be provided, if it is constant.

Width

Q_LENGTH

| Dicke | Gesamte Dicke des Fundaments, bei Streifenfundamenten horizontal senkrecht der Mittellinie. Sonst eine der beiden horizontalen Abmessungen. Der Wert wird nur angegeben, wenn die Dicke konstant ist.
| Width | Total nominal width (or thickness) of the footing. For strip footings it is measured perpendicular to the footing path (or longitudial axis). For other footings it is one of the horizontal dimensions. It should only be provided, if it is constant.

Height

Q_LENGTH

| Höhe | Höhe des Fundaments. Der Wert wird nur angegeben, wenn die Höhe konstant ist.
| Height | Total nominal height of the footing. It should only be provided, if it is constant.

CrossSectionArea

Q_AREA

| Cross Section Area | Total area of the cross section (or profile) of the footing.

OuterSurfaceArea

Q_AREA

| Outer Surface Area | Total area of the extruded surfaces of the footing (not taking into account the end cap areas), normally generated as perimeter * length.

GrossSurfaceArea

Q_AREA

| Gross Surface Area | Total area of the footing, normally generated as perimeter * length + 2 * cross section area. It is the sum of OuterSurfaceArea + (2 x CrossSectionArea) and shall only be given, if the OuterSurfaceArea and CrossSectionArea cannot be established separately.

GrossVolume

Q_VOLUME

| Gross Volume | Total gross volume of the footing, not taking into account possible processing features (cut-out's, etc.) or openings and recesses.

NetVolume

Q_VOLUME

| Net Volume | Total net volume of the footing, taking into account possible processing features (cut-out's, etc.) or openings and recesses.

GrossWeight

Q_WEIGHT

| Gross Weight | Total gross weight of the footing without add-on parts, not taking into account possible processing features (cut-out's, etc.) or openings and recesses.

NetWeight

Q_WEIGHT

| Net Weight | Total net weight of the footing without add-on parts, taking into account possible processing features (cut-out's, etc.) or openings and recesses.

Link to this page