Pset_FastenerWeld

BACnet MVD

#### 6.3.4.10 Pset_FastenerWeld

PSET_TYPEDRIVENOVERRIDE / IfcFastener / WELD

Natural language names

| Fastener Weld

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

Type1

P_SINGLEVALUE / IfcLabel

| Type1 | Type of weld seam according to ISO 2553. Note, combined welds are given by two corresponding symbols in the direction of the normal axis of the coordinate system. For example, an X weld is specified by Type1 = 'V' and Type2 = 'V'.

Type2

P_SINGLEVALUE / IfcLabel

| Type2 | See Type1.

Surface1

P_SINGLEVALUE / IfcLabel

| Surface1 | Aspect of weld seam surface, i.e. 'plane', 'curved' or 'hollow'. Combined welds are given by two corresponding symbols analogous to Type1 and Type2.

Surface2

P_SINGLEVALUE / IfcLabel

| Surface2 | See Surface1.

Process

P_SINGLEVALUE / IfcInteger

| Process | Reference number of the welding process according to ISO 4063, an up to three digits long code

ProcessName

P_SINGLEVALUE / IfcLabel

| Process Name | Name of the welding process. Alternative to the numeric Process property.

a

P_SINGLEVALUE / IfcPositiveLengthMeasure

| a | Measure a according to ISO 2553

c

P_SINGLEVALUE / IfcPositiveLengthMeasure

| c | Measure c according to ISO 2553

d

P_SINGLEVALUE / IfcPositiveLengthMeasure

| d | Measure d according to ISO 2553

e

P_SINGLEVALUE / IfcPositiveLengthMeasure

| e | Measure e according to ISO 2553

l

P_SINGLEVALUE / IfcPositiveLengthMeasure

| l | Measure l according to ISO 2553

n

P_SINGLEVALUE / IfcCountMeasure

| n | Count n according to ISO 2553

s

P_SINGLEVALUE / IfcPositiveLengthMeasure

| s | Measure s according to ISO 2553

z

P_SINGLEVALUE / IfcPositiveLengthMeasure

| z | Measure z according to ISO 2553

Intermittent

P_SINGLEVALUE / IfcBoolean

| Intermittent | If fillet weld, intermittent or not

Staggered

P_SINGLEVALUE / IfcBoolean

| Staggered | If intermittent weld, staggered or not

Link to this page