PEnum_ControllerTypeFloating

BACnet MVD

#### 7.2.4.101 PEnum_ControllerTypeFloating

Natural language names

Constants

Name | Description
--- | ---

CONSTANT

| Constant | No inputs

MODIFIER

| Modifier | Single analog input is read, added to SignalOffset, multiplied by SignalFactor, and written to the output value

ABSOLUTE

| Absolute | Single analog input is read and absolute value is written to the output value

INVERSE

| Inverse | Single analog input is read, 1

HYSTERESIS

| Hysteresis |

RUNNINGAVERAGE

| Running Average | Single analog input is read, averaged over SignalTime, and written to the output value

DERIVATIVE

| Derivative | Single analog input is read and the rate of change during the SignalTime is written to the output value

INTEGRAL

| Integral | Single analog input is read and the average value during the SignalTime is written to the output value

BINARY

| Binary | Single binary input is read and SignalOffset is written to the output value if True

ACCUMULATOR

| Accumulator | Single binary input is read, and for each pulse the SignalOffset is added to the accumulator, and while the accumulator is greater than the SignalFactor, the accumulator is decremented by SignalFactor and the integer result is incremented by one

PULSECONVERTER

| Pulse Converter | Single integer input is read, and for each increment the SignalMultiplier is added and written to the output value

LOWERLIMITCONTROL

| Lower Limit Control |

UPPERLIMITCONTROL

| Upper Limit Control |

SUM

| Sum | Two analog inputs are read, added, and written to the output value

SUBTRACT

| Subtract | Two analog inputs are read, subtracted, and written to the output value

PRODUCT

| Product | Two analog inputs are read, multiplied, and written to the output value

DIVIDE

| Divide | Two analog inputs are read, divided, and written to the output value

AVERAGE

| Average | Single analog input is read, averaged over SignalTime, and written to the output value

MAXIMUM

| Maximum | Two analog inputs are read and the maximum is written to the output value

MINIMUM

| Minimum | Two analog inputs are read and the minimum is written to the output value

REPORT

| Report |

SPLIT

| Split |

INPUT

| Input | Controller element is a dedicated input

OUTPUT

| Output | Controller element is a dedicated output

VARIABLE

| Variable | Controller element is an in-memory variable

OTHER

| (other) | Value is not listed.

NOTKNOWN

| (unknown) | Value is unknown.

UNSET

| (unset) | Value has not been specified.

References: Pset_ControllerTypeFloating

Link to this page