IfcProfileDef

BACnet MVD

#### IfcProfileDef

Natural language names

| Profil
| Profile Def
| Définition de profil

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC2x3 to IFC4
IfcProfileDef |  |  | MODIFIED | Instantiation changed from ABSTRACT.

##### Semantic definitions at the entity

Entity definition

IfcProfileDef is the supertype of all definitions of standard and arbitrary profiles within IFC. It is used to define a standard set of commonly used section profiles by their parameters or by their explicit curve geometry.

- Parameterized profiles are 2D primitives, which are used within the industry to describe cross sections by a description of its parameters.
- Arbitrary profiles are cross sections defined by an outer boundary as bounded curve, which may also include holes, defined by inner boundaries.
- Derived profiles, based on a transformation of a parent profile, are also part of the profile definitions available.
- In addition composite profiles can be defined, which include two or more profile definitions to define the resulting profile.

> HISTORY New entity in IFC1.5, the capabilities have been extended in IFC2x. Profiles can now support swept surfaces and swept area solids with inner boundaries. It had been renamed from IfcAttDrivenProfileDef.

> IFC4 CHANGE Changed from ABSTRACT to non-abstract for uses which do not require an explicitly defined geometry. Added inverse attributes HasProperties and HasExternalReference.

Use in material association

Beams, columns, and similarly shaped building elements and their type objects may be associated with a section profile definition, combined with material definition, by means of IfcRelAssociatesMaterial together with IfcMaterialProfileSet and IfcMaterialProfileSetUsage. This way, building elements and element types with same section and material can share a common section profile definition and association.

The profile definition in material association is required to be consistent with shape representations of the respective building elements.

A higher-level description of spatial aligment of the section profile of a member (such as centered, bottom-left, in the geometric centroid, and more) can be provided within IfcMaterialProfileSetUsage by means of a cardinal point reference. This can be used redundant to geometric data in order to convey design intent.

Use in shape models

Profile definitions are used within the geometry and geometric model resource to create either swept surfaces, swept area solids, or sectioned spines.

The purpose of the profile definition within the swept surfaces or swept area solids is to define a uniform cross section being swept:

- along a line (extrusion) using IfcSurfaceOfLinearExtrusion or IfcExtrudedAreaSolid
- along a circular arc (revolution) using IfcSurfaceOfRevolution or IfcRevolvedAreaSolid
- along a directrix lying on a reference surface using IfcSurfaceCurveSweptAreaSolid

The purpose of the profile definition within the sectioned spine is to define a varying cross sections at several positions along a spine curve. The subtype IfcDerivedProfileDef is particularly suited to provide the consecutive profiles to be based on transformations of the start profile and thus maintaining the identity of vertices and edges.

> NOTE Subtypes of the IfcProfileDef contain parameterized profiles (as subtypes of IfcParameterizedProfileDef) which establish their own 2D position coordinate system, profiles given by explicit curve geometry (either open or closed profiles) and two special types for composite profiles and derived profiles, based on a 2D Cartesian transformation.

An IfcProfileDef is treated as bounded area if it is used within swept area solids. In this case, the inside of the profile is part of the profile. The attribute ProfileType is set to AREA. An IfcProfileDef is treated as a curve if it is used within swept surfaces. In this case, the inside of the profile (if the curve is closed) is not part of the profile. The attribute ProfileType is set to CURVE.

Figure 368 illustrates use of parameterized profiles within a swept area solid.

Position
The IfcProfileDef is defined within the underlying coordinate system which is defined by the swept surface or swept area solid that uses the profile definition. It is the xy plane

- of IfcSweptSurface.Position or
- of IfcSweptAreaSolid.Position or
- of each list member of IfcSectionedSpine.CrossSectionPositions.

In the figure to the left, the z axis of the position coordinate system points outwards of the drawing plane.

Note: The subtype IfcParameterizedProfileDef optionally provides an additional 2D position coordinate system relative to the underlying coordinate system of the IfcProfileDef.

Sweeping

In the later use of the IfcProfileDef within the swept surface or swept area solid, e.g. the IfcExtrudedAreaSolid (here used as an example), the profile boundaries (here based on the 2D position coordinate system of IfcParameterizedProfileDef) are placed within the xy plane of the 3D position coordinate system of the swept surface or swept area solid.

The profile is inserted into the underlying coordinate system either:

- directly in case of using IfcArbitraryClosedProfileDef and IfcArbitraryOpenProfileDef,
- through an intermediate position coordinate system in case of using IfcParameterizedProfileDef.
- through an 2D Cartesian transformation operator (applied directly to the curve position when using arbitrary profile definitions, or applied to the position coordinate system when using parameterized profile definitions) in case of using IfcDerivedProfileDef.
- when using IfcCompositeProfileDef the insertion depends on the subtype of the included sub-profiles.

Figure 368 — Profile sweeping

Profile types

Results of the different usage of the ProfileType attribute are demonstrated here. The ProfileType defines whether the inside (the bounded area) is part of the profile definition (Area) or not (Curve). Figure 369 illustrates the resulting area or curve depending on ProfileType.

ProfileType = AREA | ProfileType = CURVE

Figure 369 — Profile types

Profile specification by external reference

If the profile is standardized by a norm or a catalogue, a reference to this norm or catalogue should be provided by means of HasExternalReference. This inverse relationship is used to associate an IfcExternalReference (notably IfcClassificationReference or IfcLibraryReference) with the profile.

IfcClassificationReference is used to refer to a profile norm (a common standard or manufacturer's standard). In this case,

- IfcClassificationReference.ItemReference contains the formal profile designation from the norm. (On the other hand, IfcProfileDef.ProfileName contains a displayable name which may not necessarily be the same as the formal designation.)
- IfcClassificationReference.Name carries the short name of the profile norm.
- Optionally, the norm can be further described by IfcClassificationReference.ReferencedSource.

IfcLibraryReference is used to refer to a library which contains profile definitions. In this case,

- IfcLibraryReference.ItemReference contains the identifier of the profile within the library and is meant to be machine-readable (in contrast to IfcProfileDef.ProfileName which should be human-readable).
- IfcLibraryReference.Location and .Name or .ReferencedLibrary further describe the library.

If an external reference is provided, sending systems shall ensure that the shape of the profile definition object agrees with the definitions in the referenced classification or library.

Direct instances of IfcProfileDef

Usually, only subtypes of IfcProfileDef should be instantiated. In some special cases, e.g. if the profile object is used for purposes other than geometric models (e.g. for structural analysis models), it may be possible to directly instantiate IfcProfileDef and further specify the profile only by external reference or by profile properties. The latter are tracked by the inverse attribute HasProperties.

Attribute definitions

# | Attribute | Type | Cardinality | Description | B
--- | --- | --- | --- | --- | ---
1 | ProfileType | IfcProfileTypeEnum |  | Defines the type of geometry into which this profile definition shall be resolved, either a curve or a surface area. In case of curve the profile should be referenced by a swept surface, in case of area the profile should be referenced by a swept area solid. | X | X
2 | ProfileName | IfcLabel | ? | Human-readable name of the profile, for example according to a standard profile table. As noted above, machine-readable standardized profile designations should be provided in IfcExternalReference.ItemReference. | X | X

HasExternalReference

IfcExternalReferenceRelationship
@RelatedResourceObjects

S[0:?]

Reference to external information, e.g. library, classification, or document information, which is associated with the profile.

> IFC4 CHANGE New inverse attribute

X

HasProperties

IfcProfileProperties
@ProfileDefinition

S[0:?]

Additional properties of the profile, for example mechanical properties.

> IFC4 CHANGE New inverse attribute

X

##### Inherited definitions from supertypes

Entity inheritance
Attribute inheritance

# | Attribute | Type | Cardinality | Description | B
--- | --- | --- | --- | --- | ---
IfcProfileDef
1 | ProfileType | IfcProfileTypeEnum |  | Defines the type of geometry into which this profile definition shall be resolved, either a curve or a surface area. In case of curve the profile should be referenced by a swept surface, in case of area the profile should be referenced by a swept area solid. | X | X
2 | ProfileName | IfcLabel | ? | Human-readable name of the profile, for example according to a standard profile table. As noted above, machine-readable standardized profile designations should be provided in IfcExternalReference.ItemReference. | X | X

HasExternalReference

IfcExternalReferenceRelationship
@RelatedResourceObjects

S[0:?]

Reference to external information, e.g. library, classification, or document information, which is associated with the profile.

> IFC4 CHANGE New inverse attribute

X

HasProperties

IfcProfileProperties
@ProfileDefinition

S[0:?]

Additional properties of the profile, for example mechanical properties.

> IFC4 CHANGE New inverse attribute

X

##### Formal representations

XML Specification
`<xs:element name="IfcProfileDef" type="ifc:IfcProfileDef" substitutionGroup="ifc:Entity" nillable="true"/>
<xs:complexType name="IfcProfileDef">
<xs:complexContent>
<xs:extension base="ifc:Entity">
<xs:sequence>
<xs:element name="HasProperties" nillable="true" minOccurs="0">
<xs:complexType>
<xs:sequence>
<xs:element ref="ifc:IfcProfileProperties" minOccurs="0" maxOccurs="unbounded"/>
</xs:sequence>
<xs:attribute ref="ifc:itemType" fixed="ifc:IfcProfileProperties"/>
<xs:attribute ref="ifc:cType" fixed="set"/>
<xs:attribute ref="ifc:arraySize" use="optional"/>
</xs:complexType>
</xs:element>
</xs:sequence>
<xs:attribute name="ProfileType" type="ifc:IfcProfileTypeEnum" use="optional"/>
<xs:attribute name="ProfileName" type="ifc:IfcLabel" use="optional"/>
</xs:extension>
</xs:complexContent>
</xs:complexType>
`
EXPRESS Specification
`ENTITY IfcProfileDef
SUPERTYPE OF(ONEOF(IfcArbitraryClosedProfileDef, IfcArbitraryOpenProfileDef, IfcCompositeProfileDef, IfcDerivedProfileDef, IfcParameterizedProfileDef));
ProfileType : IfcProfileTypeEnum;
ProfileName : OPTIONAL IfcLabel;
INVERSE
HasExternalReference : SET [0:?] OF IfcExternalReferenceRelationship FOR RelatedResourceObjects;
HasProperties : SET [0:?] OF IfcProfileProperties FOR ProfileDefinition;
END_ENTITY;

EXPRESS-G diagram

`

References: IfcResourceObjectSelect IfcExtrudedAreaSolidTapered IfcRevolvedAreaSolidTapered IfcSectionedSpine IfcSweptAreaSolid IfcSweptSurface IfcMaterialProfile IfcCompositeProfileDef IfcDerivedProfileDef IfcProfileProperties IfcSectionProperties

Link to this page