Pset_SwitchingDeviceTypeSwitchDisconnector

BACnet MVD

#### 7.4.4.78 Pset_SwitchingDeviceTypeSwitchDisconnector

PSET_TYPEDRIVENOVERRIDE / IfcSwitchingDevice / SWITCHDISCONNECTOR

Natural language names

| Switching Device Type Switch Disconnector

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

SwitchDisconnectorType

P_ENUMERATEDVALUE / IfcLabel / PEnum_SwitchDisconnectorType

| Switch Disconnector Type | A list of the available types of switch disconnector from which that required may be selected where: CenterBreak: A disconnector in which both contacts of each pole are movable and engage at a point substantially midway between their supports. (IEC 441-14-08) DividedSupport: A disconnector in which the fixed and moving contacts of each pole are not supported by a common base or frame. (IEC 441-14-06) DoubleBreak: A disconnector that opens a circuit at two points. (IEC 441-14-09) EarthingSwitch: A disconnector in which the fixed and moving contacts of each pole are not supported by a common base or frame. (IEC 441-14-07) Isolator: A disconnector which in the open position satisfies isolating requirements. (IEC 441-14-12)
| 高圧遮断機タイプ | 以下より選択が必要となる、スイッチ断路機の一覧リスト： センターブレイク： 各極の両方の接点は可動式で、実質的に中間付近を保持する断路器。 (IEC 441-14-08) DividedSupport： 各極の固定側と移動側接点が、共通のベースまたはフレームではサポートされない断路器。(IEC 441-14-06) 二点切り断路器： 2点で回路を開く断路器 (IEC 441-14-09) 接地開閉器 ： 各極の固定側と移動側接点が、共通のベースまたはフレームではサポートされない断路器。(IEC 441-14-07) 断路器： 解放位置の分離要件を満たす、断路器。(IEC 441-14-12)

LoadDisconnectionType

P_ENUMERATEDVALUE / IfcLabel / PEnum_LoadDisconnectionType

| Load Disconnection Type | A list of the available types of load disconnection from which that required may be selected.
| 切断タイプ | 選択が必要となる、負荷開閉器タイプの一覧リスト。

Link to this page