Pset_SpaceThermalDesign

BACnet MVD

#### 6.2.4.24 Pset_SpaceThermalDesign

PSET_TYPEDRIVENOVERRIDE / IfcSpace

Natural language names

| Space Thermal Design

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

CoolingDesignAirflow

P_SINGLEVALUE / IfcVolumetricFlowRateMeasure

| Cooling Design Airflow | The air flowrate required during the peak cooling conditions.
| 冷房設計吸気量 | ピーク時の冷房条件で要求される給気量。

HeatingDesignAirflow

P_SINGLEVALUE / IfcVolumetricFlowRateMeasure

| Heating Design Airflow | The air flowrate required during the peak heating conditions, but could also be determined by minimum ventilation requirement or minimum air change requirements.

TotalSensibleHeatGain

P_SINGLEVALUE / IfcPowerMeasure

| Total Sensible Heat Gain | The total sensible heat or energy gained by the space during the peak cooling conditions.
| 顕熱負荷の合計 | ピーク時の冷房条件で取得した顕熱或いはエネルギー。

TotalHeatGain

P_SINGLEVALUE / IfcPowerMeasure

| Total Heat Gain | The total amount of heat or energy gained by the space at the time of the space's peak cooling conditions.
| 熱取得の合計 | ピーク時の室内最大冷房負荷時に取得した顕熱或いはエネルギー。

TotalHeatLoss

P_SINGLEVALUE / IfcPowerMeasure

| Total Heat Loss | The total amount of heat or energy lost by the space at the time of the space's peak heating conditions.
| 熱ロスの合計 | ピーク時の室内最大暖房負荷時に取得・損失した熱或いはエネルギー。

CoolingDryBulb

P_SINGLEVALUE / IfcThermodynamicTemperatureMeasure

| Cooling Dry Bulb | Inside dry bulb temperature for cooling design.
| 冷房設計温度 | 冷房設計における室内設計乾球温度。

CoolingRelativeHumidity

P_SINGLEVALUE / IfcPositiveRatioMeasure

| Cooling Relative Humidity | Inside relative humidity for cooling design.
| 冷房設計相対湿度 | 冷房設計における室内設計相対湿度。

HeatingDryBulb

P_SINGLEVALUE / IfcThermodynamicTemperatureMeasure

| Heating Dry Bulb | Inside dry bulb temperature for heating design.
| 暖房設計温度 | 暖房設計における室内設計乾球温度。

HeatingRelativeHumidity

P_SINGLEVALUE / IfcPositiveRatioMeasure

| Heating Relative Humidity | Inside relative humidity for heating design.
| 暖房設計相対湿度 | 暖房設計における室内設計相対湿度。

VentilationAirFlowrate

P_SINGLEVALUE / IfcVolumetricFlowRateMeasure

| Ventilation Air Flowrate | Ventilation outside air requirement for the space.
| 外気量 | 必要外気量。

ExhaustAirFlowrate

P_SINGLEVALUE / IfcVolumetricFlowRateMeasure

| Exhaust Air Flowrate | Design exhaust air flow rate for the space.
| 排気量 | 設計排気量。

CeilingRAPlenum

P_SINGLEVALUE / IfcBoolean

| Ceiling RAPlenum | Ceiling plenum used for return air or not. TRUE = Yes, FALSE = No.
| 天井裏還気 | 天井裏還気（リタンあり・なし）　TRUE=あり、FALSE=なし。

BoundaryAreaHeatLoss

P_SINGLEVALUE / IfcHeatFluxDensityMeasure

| Boundary Area Heat Loss | Heat loss per unit area for the boundary object. This is a design input value for use in the absence of calculated load data.
| 周辺関連設備の熱ロス | 単位面積ありた周辺関連設備の熱ロス。空調負荷計算値以外の設計設定値。

Link to this page