PEnum_ControllerTwoPositionType

BACnet MVD

#### 7.2.4.100 PEnum_ControllerTwoPositionType

Natural language names

Constants

Name | Description
--- | ---

NOT

| Not | Single binary input is read and the opposite value is written to the output value

AND

| And | Two binary inputs are read and if both are True then True is written to the output value

OR

| Or | Two binary inputs are read and if either is True then True is written to the output value

XOR

| Xor | Two binary inputs are read and if one is true then True is written to the output value

LOWERLIMITSWITCH

| Lower Limit Switch | Single analog input is read and if less than Value

UPPERLIMITSWITCH

| Upper Limit Switch | Single analog input is read and if more than Value

LOWERBANDSWITCH

| Lower Band Switch | Single analog input is read and if less than Value

UPPERBANDSWITCH

| Upper Band Switch | Single analog input is read and if more than Value

AVERAGE

| Average |

CALENDAR

| Calendar | No inputs

INPUT

| Input | Controller element is a dedicated input

OUTPUT

| Output | Controller element is a dedicated output

VARIABLE

| Variable | Controller element is an in-memory variable

OTHER

| (other) | Value is not listed.

NOTKNOWN

| (unknown) | Value is unknown.

UNSET

| (unset) | Value has not been specified.

References: Pset_ControllerTypeTwoPosition

Link to this page