Pset_SwitchingDeviceTypeStarter

BACnet MVD

#### 7.4.4.77 Pset_SwitchingDeviceTypeStarter

PSET_TYPEDRIVENOVERRIDE / IfcSwitchingDevice / STARTER

Natural language names

| Switching Device Type Starter

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

StarterType

P_ENUMERATEDVALUE / IfcLabel / PEnum_StarterType

| Starter Type | A list of the available types of starter from which that required may be selected where: AutoTransformer: A starter for an induction motor which uses for starting one or more reduced voltages derived from an auto transformer. (IEC 441-14-45) Manual: A starter in which the force for closing the main contacts is provided exclusively by manual energy. (IEC 441-14-39) DirectOnLine: A starter which connects the line voltage across the motor terminals in one step. (IEC 441-14-40) Frequency: A starter in which the frequency of the power supply is progressively increased until the normal operation frequency is attained. nStep: A starter in which there are (n-1) intermediate accelerating positions between the off and full on positions. (IEC 441-14-41) Rheostatic: A starter using one or several resistors for obtaining, during starting, stated motor torque characteristics and for limiting the current. (IEC 441-14-425) StarDelta: A starter for a 3 phase induction motor such that in the starting position the stator windings are connected in star and in the final running position they are connected in delta. (IEC 441-14-44)
| 始動タイプ | 以下より選択が必要となる、始動の一覧リスト： 自動： 自動トランスから引き出された１つ以上の低下した電圧でスタートするために使用する誘導電動機用のスターター (IEC 441-14-45) 手動： メインのコンタクトから強制的に分離されたところにあり、手動によりエネルギーが供給される (IEC 441-14-39) じか入れ: ワンステップでモーター・ターミナル間の線間電圧をつなぐスターター (IEC 441-14-40) 振動：電源の振動数が通常の操作振動まで次第に増大して行くスターター nStep: オフ（OFF)とオン（ON）の間で、（n-1）の中間の加速度的な位置であるスターター。 (IEC 441-14-41) 抵抗：モータのトルク特性の取得、開始、そして安定する間に、電流を制限するために 1 つまたはいくつかの抵抗を利用したスターター (IEC 441-14-425) スターデルタ：開始位置では固定小巻線（スターターワインディング）が星状で接続され、その後、最終の実行状態ではデルタ状に接続されるという3相誘導モーター用のスターター。（IEC 441-14-44）

Link to this page