Pset_SanitaryTerminalTypeBidet

BACnet MVD

#### 7.6.4.8 Pset_SanitaryTerminalTypeBidet

PSET_TYPEDRIVENOVERRIDE / IfcSanitaryTerminal / BIDET

Natural language names

| Sanitary Terminal Type Bidet

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC4 Addendum 2
Pset_SanitaryTerminalTypeBidet |  |  |  |
NominalLength |  |  | DELETED |
NominalWidth |  |  | DELETED |
NominalDepth |  |  | DELETED |
Color |  |  | DELETED |

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

Mounting

P_ENUMERATEDVALUE / IfcLabel / PEnum_SanitaryMounting

| Mounting | The property enumeration Pset_SanitaryMountingEnum defines the forms of mounting or fixing of the sanitary terminal that may be specified within property sets used to define sanitary terminals (WC’s, basins, sinks, etc.) where:- BackToWall: A pedestal mounted sanitary terminal that fits flush to the wall at the rear to cover its service connections . Pedestal: A floor mounted sanitary terminal that has an integral base . CounterTop: A sanitary terminal that is installed into a horizontal surface that is installed into a horizontal surface. Note: When applied to a wash hand basin, the term more normally used is ‘vanity’. See also Wash Hand Basin Type specification. WallHung: A sanitary terminal cantilevered clear of the floor. Note that BackToWall, Pedestal and WallHung are allowable values for a bidet.
| 装着 | 列挙するプロパティはPset_SanitaryMountingEnumでは（トイレの、洗面台、シンクなど）、衛生配管への装着法で定義される： 床置き壁排水：台座は、カバーの背面の壁にあるフラッシュバルブに接続される。 床置き：床の衛生配管に装着される。 カウンター：水平面に設置された衛生配管に接続します。注：手洗器があると、通常は'化粧'が使用される。手洗器を参照。 壁掛け：衛生配管は壁から出され床には何もなくなる。。 床置き壁排水、床置き、壁掛けは、ビデの許容値であることに注意。

SpilloverLevel

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Spillover Level | The level at which water spills out of the object.
| 流出レベル | 水がこぼれるレベル。

DrainSize

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Drain Size | The size of the drain outlet connection from the object.
| ドレインサイズ | 排水口の接続のサイズ。

Link to this page