IfcCableFittingTypeEnum

BACnet MVD

#### IfcCableFittingTypeEnum

Natural language names

| Cable Fitting Type Enum
| Enumération des types de raccord de câble

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC2x3 to IFC4
IfcCableFittingTypeEnum |  |  | ADDED |

##### Semantic definitions at the type

Type definition

The IfcCableFittingTypeEnum defines the range of different types of cable fitting that can be specified.

> HISTORY New type in IFC4.

Enumeration definition

Constant | Description
--- | ---
CONNECTOR | A fitting that joins two cable segments of the same connector type (though potentially different gender).
ENTRY | A fitting that begins a cable segment at a non-electrical element such as a grounding clamp attached to a pipe.
EXIT | A fitting that ends a cable segment at a non-electrical element such as a grounding clamp attached to a pipe or to the ground.
JUNCTION | A fitting that joins three or more segments of arbitrary connector types for signal splitting or multiplexing.
TRANSITION | A fitting that joins two cable segments of different connector types.
USERDEFINED | User-defined type.
NOTDEFINED | Undefined type.

##### Formal representations

XML Specification
`<xs:simpleType name="IfcCableFittingTypeEnum">
<xs:restriction base="xs:string">
<xs:enumeration value="connector"/>
<xs:enumeration value="entry"/>
<xs:enumeration value="exit"/>
<xs:enumeration value="junction"/>
<xs:enumeration value="transition"/>
<xs:enumeration value="userdefined"/>
<xs:enumeration value="notdefined"/>
</xs:restriction>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcCableFittingTypeEnum = ENUMERATION OF (
CONNECTOR,
ENTRY,
EXIT,
JUNCTION,
TRANSITION,
USERDEFINED,
NOTDEFINED);
END_TYPE;

EXPRESS-G diagram

`

References: IfcCableFitting IfcCableFittingType

Link to this page