IfcOutletTypeEnum

BACnet MVD

#### IfcOutletTypeEnum

Natural language names

| Outlet Type Enum
| Enumération des types de prise

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC2x3 to IFC4
IfcOutletTypeEnum |  |  |  |
DATAOUTLET |  |  | ADDED |
TELEPHONEOUTLET |  |  | ADDED |

##### Semantic definitions at the type

Type definition

The IfcOutletTypeEnum defines the range of different types of outlet that can be specified.

> HISTORY New type in IFC2x.

> IFC4 CHANGE Telephone and Data outlets added.

Enumeration definition

Constant | Description
--- | ---
AUDIOVISUALOUTLET | An outlet used for an audio or visual device.
COMMUNICATIONSOUTLET | An outlet used for connecting communications equipment.
POWEROUTLET | An outlet used for connecting electrical devices requiring power.
DATAOUTLET | An outlet used for connecting data communications equipment.
TELEPHONEOUTLET | An outlet used for connecting telephone communications equipment.
USERDEFINED | User-defined type.
NOTDEFINED | Undefined type.<

##### Formal representations

XML Specification
`<xs:simpleType name="IfcOutletTypeEnum">
<xs:restriction base="xs:string">
<xs:enumeration value="audiovisualoutlet"/>
<xs:enumeration value="communicationsoutlet"/>
<xs:enumeration value="poweroutlet"/>
<xs:enumeration value="dataoutlet"/>
<xs:enumeration value="telephoneoutlet"/>
<xs:enumeration value="userdefined"/>
<xs:enumeration value="notdefined"/>
</xs:restriction>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcOutletTypeEnum = ENUMERATION OF (
AUDIOVISUALOUTLET,
COMMUNICATIONSOUTLET,
POWEROUTLET,
DATAOUTLET,
TELEPHONEOUTLET,
USERDEFINED,
NOTDEFINED);
END_TYPE;

EXPRESS-G diagram

`

References: IfcOutlet IfcOutletType

Link to this page