Pset_MaterialWoodBasedPanel

BACnet MVD

#### 8.10.5.14 Pset_MaterialWoodBasedPanel

PSET_TYPEDRIVENOVERRIDE / IfcMaterial / Wood

Natural language names

| Material Wood Based Panel

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

ApplicableStructuralDesignMethod

P_SINGLEVALUE / IfcLabel

| Applicable Structural Design Method | Determines whether mechanical material properties are applicable to 'ASD' = allowable stress design (working stress design), 'LSD' = limit state design, or 'LRFD' = load and resistance factor design.

InPlane

COMPLEX / CP_MaterialMechanicalPanel

| In Plane | Mechanical properties with respect to in-plane load, i.e. for function as a membrane.

Name | Type | Description
--- | --- | ---
YoungModulusBending | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcModulusOfElasticityMeasure | Defining values: α; defined values: elastic modulus in bending.
YoungModulusTension | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcModulusOfElasticityMeasure | Defining values: α; defined values: elastic modulus in tension.
YoungModulusCompression | P_SINGLEVALUE / IfcModulusOfElasticityMeasure | Elastic modulus in compression.
ShearModulus | P_SINGLEVALUE / IfcModulusOfElasticityMeasure | Shear modulus.
BendingStrength | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcPressureMeasure | Defining values: α; defined values: bending strength.
CompressiveStrength | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcPressureMeasure | Defining values: α; defined values: compressive strength.
TensileStrength | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcPressureMeasure | Defining values: α; defined values: tensile strength.
ShearStrength | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcPressureMeasure | Defining values: α; defined values: shear strength.
BearingStrength | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcPressureMeasure | Defining values: α; defined values: bearing strength of bolt holes, i.e. intrados pressure.
RaisedCompressiveStrength | P_SINGLEVALUE / IfcPressureMeasure | Alternative value for compressive strength which may be used under material and code dependent conditions (e.g. if deformation is tolerable, or far from ends of the member); conditions should be stated in SELF\IfcProperty.Description.
ReferenceDepth | P_SINGLEVALUE / IfcPositiveLengthMeasure | Depth in bending for which the mechanical properties are valid; provided as a means to check the integrity of material assignment.

OutOfPlane

COMPLEX / CP_MaterialMechanicalPanel

| Out Of Plane | Mechanical properties with respect to out-of-plane load, i.e. for function as a plate; tension zone of unbalanced layups is stressed in tension.

Name | Type | Description
--- | --- | ---
YoungModulusBending | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcModulusOfElasticityMeasure | Defining values: α; defined values: elastic modulus in bending.
YoungModulusTension | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcModulusOfElasticityMeasure | Defining values: α; defined values: elastic modulus in tension.
YoungModulusCompression | P_SINGLEVALUE / IfcModulusOfElasticityMeasure | Elastic modulus in compression.
ShearModulus | P_SINGLEVALUE / IfcModulusOfElasticityMeasure | Shear modulus.
BendingStrength | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcPressureMeasure | Defining values: α; defined values: bending strength.
CompressiveStrength | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcPressureMeasure | Defining values: α; defined values: compressive strength.
TensileStrength | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcPressureMeasure | Defining values: α; defined values: tensile strength.
ShearStrength | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcPressureMeasure | Defining values: α; defined values: shear strength.
BearingStrength | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcPressureMeasure | Defining values: α; defined values: bearing strength of bolt holes, i.e. intrados pressure.
RaisedCompressiveStrength | P_SINGLEVALUE / IfcPressureMeasure | Alternative value for compressive strength which may be used under material and code dependent conditions (e.g. if deformation is tolerable, or far from ends of the member); conditions should be stated in SELF\IfcProperty.Description.
ReferenceDepth | P_SINGLEVALUE / IfcPositiveLengthMeasure | Depth in bending for which the mechanical properties are valid; provided as a means to check the integrity of material assignment.

OutOfPlaneNegative

COMPLEX / CP_MaterialMechanicalPanel

| Out Of Plane Negative | Mechanical properties with respect to out-of-plane load i.e. for function as a plate; compression zone of unbalanced layups is stressed in tension.

Name | Type | Description
--- | --- | ---
YoungModulusBending | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcModulusOfElasticityMeasure | Defining values: α; defined values: elastic modulus in bending.
YoungModulusTension | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcModulusOfElasticityMeasure | Defining values: α; defined values: elastic modulus in tension.
YoungModulusCompression | P_SINGLEVALUE / IfcModulusOfElasticityMeasure | Elastic modulus in compression.
ShearModulus | P_SINGLEVALUE / IfcModulusOfElasticityMeasure | Shear modulus.
BendingStrength | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcPressureMeasure | Defining values: α; defined values: bending strength.
CompressiveStrength | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcPressureMeasure | Defining values: α; defined values: compressive strength.
TensileStrength | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcPressureMeasure | Defining values: α; defined values: tensile strength.
ShearStrength | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcPressureMeasure | Defining values: α; defined values: shear strength.
BearingStrength | P_TABLEVALUE / IfcPositivePlaneAngleMeasure / IfcPressureMeasure | Defining values: α; defined values: bearing strength of bolt holes, i.e. intrados pressure.
RaisedCompressiveStrength | P_SINGLEVALUE / IfcPressureMeasure | Alternative value for compressive strength which may be used under material and code dependent conditions (e.g. if deformation is tolerable, or far from ends of the member); conditions should be stated in SELF\IfcProperty.Description.
ReferenceDepth | P_SINGLEVALUE / IfcPositiveLengthMeasure | Depth in bending for which the mechanical properties are valid; provided as a means to check the integrity of material assignment.

Link to this page