PEnum_DistributionPortElectricalType

BACnet MVD

#### 6.2.4.34 PEnum_DistributionPortElectricalType

Natural language names

Constants

Name | Description
--- | ---

ACPLUG

| AC Plug | AC plug

DCPLUG

| DC Plug | DC plug

COAXIAL

| Coaxial | Coaxial cable for high-speed communication

CRIMP

| Crimp | Crimped wire

RJ

| Rj | Registered jack

RADIO

| Radio | Radio wave transmission

DIN

| DIN |

DSUB

| D-Sub |

DVI

| DVI | Digital video interchange

EIAJ

| EIAJ |

HDMI

| HDMI | High-definition multimedia interface

RCA

| RCA |

SOCKET | Socket for a light bulb, where the ConnectionSubtype identifies the base (though not necessarily the bulb shape or size).

TRS

| TRS |

USB

| USB |

XLR

| XLR |

OTHER

| (other) | Value is not listed.

NOTKNOWN

| (unknown) | Value is unknown.

UNSET

| (unset) | Value has not been specified.

References: Pset_DistributionPortTypeCable

Link to this page