Pset_SpaceThermalLoadPHistory

BACnet MVD

#### 6.2.4.26 Pset_SpaceThermalLoadPHistory

PSET_PERFORMANCEDRIVEN / IfcSpace

Natural language names

| Space Thermal Load PHistory

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

People

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| People | Heat gains and losses from people.
| 人員 | 人員からの熱取得。

Lighting

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Lighting | Lighting loads.
| 照明 | 照明負荷。

EquipmentSensible

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Equipment Sensible | Heat gains and losses from equipment.
| 事務機器の顕熱 | 事務機器からの熱取得と熱ロス。

VentilationIndoorAir

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Ventilation Indoor Air | Ventilation loads from indoor air.
| 室内の換気量 | 室内の換気による熱負荷。

VentilationOutdoorAir

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Ventilation Outdoor Air | Ventilation loads from outdoor air.
| 外気量 | 外気による熱負荷。

RecirculatedAir

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Recirculated Air | Loads from recirculated air.
| 循環空気 | 循環空気による熱負荷。

ExhaustAir

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Exhaust Air | Loads from exhaust air.
| 排気 | 排気による熱負荷。

AirExchangeRate

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Air Exchange Rate | Loads from the air exchange rate.
| 換気回数 | 換気による熱負荷。

DryBulbTemperature

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Dry Bulb Temperature | Loads from the dry bulb temperature.
| 乾球温度 | 乾球温度による熱負荷。

RelativeHumidity

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Relative Humidity | Loads from the relative humidity.
| 相対湿度 | 相対湿度による熱負荷。

InfiltrationSensible

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Infiltration Sensible | Heat gains and losses from infiltration.
| すき間風の顕熱 | すき間風からの熱負荷と熱ロス。

TotalSensibleLoad

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Total Sensible Load | Total energy added or removed from air that affects its temperature. If a value is less than zero (negative), then the thermal load is lost from the space. If a value is greater than zero (positive), then the thermal load is a gain to the space.
| 顕熱負荷の合計 | 空気温度を上昇・下降させる取得・損失の熱量の合計。ゼロより小さい（－）場合、室内が熱損失となる。ゼロより大きい（＋）場合、室内が熱取得となる。

TotalLatentLoad

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Total Latent Load | Total energy added or removed from air that affects its humidity or concentration of water vapor. If a value is less than zero (negative), then the thermal load is lost from the space. If a value is greater than zero (positive), then the thermal load is a gain to the space.
| 潜熱負荷の合計 | 空気湿度（水蒸気量）を上昇・下降させる取得・損失の熱量の合計。ゼロより小さい（－）場合、室内の水蒸気が減少となる。ゼロより大きい（＋）場合、室内の水蒸気が増大となる。

TotalRadiantLoad

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Total Radiant Load | Total electromagnetic energy added or removed by emission or absorption. If a value is less than zero (negative), then the thermal load is lost from the space. If a value is greater than zero (positive), then the thermal load is a gain to the space.
| 放射熱負荷の合計 | 放射や吸収による放射エネルギーの増加、或いは減少の合計。ゼロより小さい（－）場合、放射エネルギーが減少となる。ゼロより大きい（＋）場合、放射エネルギーが増大となる。

Link to this page