Pset_FilterTypeCompressedAirFilter

BACnet MVD

#### 7.5.4.56 Pset_FilterTypeCompressedAirFilter

PSET_TYPEDRIVENOVERRIDE / IfcFilter / COMPRESSEDAIRFILTER

Natural language names

| Filter Type Compressed Air Filter

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

CompressedAirFilterType

P_ENUMERATEDVALUE / IfcLabel / PEnum_CompressedAirFilterType

| Compressed Air Filter Type | ACTIVATEDCARBON: absorbs oil vapor and odor; PARTICLE_FILTER: used to absorb solid particles of medium size; COALESCENSE_FILTER: used to absorb fine solid, oil, and water particles, also called micro filter

OperationPressureMax

P_SINGLEVALUE / IfcPressureMeasure

| Operation Pressure Max | Maximum pressure under normal operating conditions.

ParticleAbsorptionCurve

P_TABLEVALUE / IfcPositiveLengthMeasure / IfcPositiveRatioMeasure

| Particle Absorption Curve | Ratio of particles that are removed by the filter. Each entry describes the ratio of particles absorbed greater than equal to the specified size and less than the next specified size. For example, given for 3 significant particle sizes >= 0,1 micro m, >= 1 micro m, >= 5 micro m

AutomaticCondensateDischarge

P_SINGLEVALUE / IfcBoolean

| Automatic Condensate Discharge | Whether or not the condensing water or oil is discharged automatically from the filter.

CloggingIndicator

P_SINGLEVALUE / IfcBoolean

| Clogging Indicator | Whether the filter has an indicator to display the degree of clogging of the filter.

Link to this page