**Highlights**

(1) Two different fatigue initiation mechanisms are summarized for the Al-Si piston alloys at different temperatures.

(2) The relationship between fatigue life and temperature is established based the energy-based fatigue model.

(3) An optimization strategy is proposed for fatigue property optimization.

(4) The remarkable improvement of the fatigue properties is achieved with ultrasonic melt treatment.