IfcCondenserTypeEnum

BACnet MVD

#### IfcCondenserTypeEnum

Natural language names

| Condenser Type Enum
| Énumération des types de condenseur

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC2x3 to IFC4
IfcCondenserTypeEnum |  |  |  |
WATERCOOLED |  |  | ADDED |

##### Semantic definitions at the type

Type definition

Enumeration defining the typical types of condensers. Air is used as the cooling medium for AIRCOOLED; water is used as the cooling medium for all other types.

> HISTORY New enumeration in IFC2x2. WATERCOOLED added in IFC4.

Enumeration definition

Constant | Description
--- | ---
AIRCOOLED | A condenser in which heat is transferred to an air-stream.
EVAPORATIVECOOLED | A condenser that is cooled evaporatively.
WATERCOOLED | Water-cooled condenser with unspecified operation.
WATERCOOLEDBRAZEDPLATE | Water-cooled condenser with plates brazed together to form an assembly of separate channels.
WATERCOOLEDSHELLCOIL | Water-cooled condenser with cooling water circulated through one or more continuous or assembled coils contained within the shell.
WATERCOOLEDSHELLTUBE | Water-cooled condenser with cooling water circulated through one or more tubes contained within the shell.
WATERCOOLEDTUBEINTUBE | Water-cooled condenser consisting of one or more assemblies of two tubes, one within the other.
USERDEFINED | User-defined condenser type.
NOTDEFINED | Undefined condenser type.

##### Formal representations

XML Specification
`<xs:simpleType name="IfcCondenserTypeEnum">
<xs:restriction base="xs:string">
<xs:enumeration value="aircooled"/>
<xs:enumeration value="evaporativecooled"/>
<xs:enumeration value="watercooled"/>
<xs:enumeration value="watercooledbrazedplate"/>
<xs:enumeration value="watercooledshellcoil"/>
<xs:enumeration value="watercooledshelltube"/>
<xs:enumeration value="watercooledtubeintube"/>
<xs:enumeration value="userdefined"/>
<xs:enumeration value="notdefined"/>
</xs:restriction>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcCondenserTypeEnum = ENUMERATION OF (
AIRCOOLED,
EVAPORATIVECOOLED,
WATERCOOLED,
WATERCOOLEDBRAZEDPLATE,
WATERCOOLEDSHELLCOIL,
WATERCOOLEDSHELLTUBE,
WATERCOOLEDTUBEINTUBE,
USERDEFINED,
NOTDEFINED);
END_TYPE;

EXPRESS-G diagram

`

References: IfcCondenser IfcCondenserType

Link to this page