IfcElectricGeneratorTypeEnum

BACnet MVD

#### IfcElectricGeneratorTypeEnum

Natural language names

| Electric Generator Type Enum
| Enumération des types de générateur électrique

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC2x3 to IFC4
IfcElectricGeneratorTypeEnum |  |  |  |
CHP |  |  | ADDED |
ENGINEGENERATOR |  |  | ADDED |
STANDALONE |  |  | ADDED |

##### Semantic definitions at the type

Type definition

The IfcElectricGeneratorTypeEnum defines different types of electric generators.

> HISTORY New type in IFC2x2. Values added in IFC4.

Enumeration definition

Constant | Description
--- | ---
CHP | Combined heat and power supply, used not only as a source of electric energy but also as a heating source for the building. It may therefore be not only part of an electrical system but also of a heating system.
ENGINEGENERATOR | Electrical generator with a fuel-driven engine, for example a diesel-driven emergency power supply.
STANDALONE | Electrical generator which does not include its source of kinetic energy, that is, a motor, engine, or turbine are all modeled separately.
USERDEFINED | User-defined type.
NOTDEFINED | Undefined type.

##### Formal representations

XML Specification
`<xs:simpleType name="IfcElectricGeneratorTypeEnum">
<xs:restriction base="xs:string">
<xs:enumeration value="chp"/>
<xs:enumeration value="enginegenerator"/>
<xs:enumeration value="standalone"/>
<xs:enumeration value="userdefined"/>
<xs:enumeration value="notdefined"/>
</xs:restriction>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcElectricGeneratorTypeEnum = ENUMERATION OF (
CHP,
ENGINEGENERATOR,
STANDALONE,
USERDEFINED,
NOTDEFINED);
END_TYPE;

EXPRESS-G diagram

`

References: IfcElectricGenerator IfcElectricGeneratorType

Link to this page