IfcThermalAdmittanceMeasure

BACnet MVD

#### IfcThermalAdmittanceMeasure

Natural language names

| Thermal Admittance Measure
| Mesure d'admittance thermique

##### Semantic definitions at the type

Type definition

IfcThermalAdmittanceMeasure is the measure of the ability of a surface to smooth out temperature variations.

Usually measured in Watt / m2 Kelvin.

Type: REAL

> HISTORY New type in IFC2.0.

##### Formal representations

XML Specification
`<xs:simpleType name="IfcThermalAdmittanceMeasure">
<xs:restriction base="xs:double"/>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcThermalAdmittanceMeasure = REAL;
END_TYPE;

EXPRESS-G diagram

`

References: IfcDerivedMeasureValue

Link to this page