Pset_SanitaryTerminalTypeBath

BACnet MVD

#### 7.6.4.7 Pset_SanitaryTerminalTypeBath

PSET_TYPEDRIVENOVERRIDE / IfcSanitaryTerminal / BATH

Natural language names

| Sanitary Terminal Type Bath

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC4 Addendum 2
Pset_SanitaryTerminalTypeBath |  |  |  |
NominalLength |  |  | DELETED |
NominalWidth |  |  | DELETED |
NominalDepth |  |  | DELETED |
Color |  |  | DELETED |

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

BathType

P_ENUMERATEDVALUE / IfcLabel / PEnum_BathType

| Bath Type | The property enumeration defines the types of bath that may be specified within the property set.
| バスタイプ | 列挙するプロパティは、プロパティセット内で指定することができるバスの種類の定義： 家庭用：全身を簡単に浸漬することができる一度に1人の人間が入るバス。 家庭用Corner：浸漬トラフが傾いていて、全身を簡単に浸漬することができる一度に1人の人間が入るバス。 フットバス：足を洗う浅いバス。 ジャグジー：複数の人のための渦のバス プランジバス：通常は全身を簡単に浸漬することができまる一度に複数の人の入るバス。 座バス：水浴を椅子のように座って行うバス。 治療バス：水浴セラピーの目的に使用されるバス。 渦バス：ポンプによる水の循環や、水や空気の誘引により水を攪拌する統合された装置としてのバス。

DrainSize

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Drain Size | The size of the drain outlet connection from the object.
| ドレインサイズ | 排水口の接続のサイズ。

HasGrabHandles

P_SINGLEVALUE / IfcBoolean

| Has Grab Handles | Indicates whether the bath is fitted with handles that provide assistance to a bather in entering or leaving the bath.
| 手すりの有無 | 風呂の出入りを補助する手すりが取り付けられているかどうかを示す。

Link to this page