PEnum_ValvePattern

BACnet MVD

#### 7.5.4.201 PEnum_ValvePattern

Natural language names

Constants

Name | Description
--- | ---

SINGLEPORT

| Single Port | Valve that has a single entry port from the system that it serves, the exit port being to the surrounding environment

ANGLED_2_PORT

| Angled 2 Port | Valve in which the direction of flow is changed through 90 degrees

STRAIGHT_2_PORT

| Straight 2 Port | Valve in which the flow is straight through

STRAIGHT_3_PORT

| Straight 3 Port | Valve with three separate ports

CROSSOVER_4_PORT

| Crossover 4 Port | Valve with 4 separate ports

OTHER

| (other) | Value is not listed.

NOTKNOWN

| (unknown) | Value is unknown.

UNSET

| (unset) | Value has not been specified.

References: Pset_ValveTypeCommon

Link to this page