Pset_MaterialFuel

BACnet MVD

#### 8.10.5.5 Pset_MaterialFuel

PSET_TYPEDRIVENOVERRIDE / IfcMaterial

Natural language names

| Material Fuel

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

CombustionTemperature

P_SINGLEVALUE / IfcThermodynamicTemperatureMeasure

| Combustion Temperature | Combustion temperature of the material when air is at 298 K and 100 kPa.

CarbonContent

P_SINGLEVALUE / IfcPositiveRatioMeasure

| Carbon Content | The carbon content in the fuel. This is measured in weight of carbon per unit weight of fuel and is therefore unitless.

LowerHeatingValue

P_SINGLEVALUE / IfcHeatingValueMeasure

| Lower Heating Value | Lower Heating Value is defined as the amount of energy released (MJ/kg) when a fuel is burned completely, and H2O is in vapor form in the combustion products.

HigherHeatingValue

P_SINGLEVALUE / IfcHeatingValueMeasure

| Higher Heating Value | Higher Heating Value is defined as the amount of energy released (MJ/kg) when a fuel is burned completely, and H2O is in liquid form in the combustion products.

Link to this page