Pset_ProtectiveDeviceTrippingUnitTypeResidualCurrent

BACnet MVD

#### 7.4.4.59 Pset_ProtectiveDeviceTrippingUnitTypeResidualCurrent

PSET_TYPEDRIVENOVERRIDE / IfcProtectiveDeviceTrippingUnit / RESIDUALCURRENT

Natural language names

| Protective Device Tripping Unit Type Residual Current

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

TrippingUnitReleaseCurrent

P_ENUMERATEDVALUE / IfcLabel / PEnum_TrippingUnitReleaseCurrent

| Tripping Unit Release Current | The value of tripping or residual current for which the device has the possibility to be equipped. The values are given in mA.
| 定格感度電流 | 漏電ブレーカの感度電流値（mA）。

Link to this page