PEnum_AirSideSystemType

BACnet MVD

#### 6.2.4.31 PEnum_AirSideSystemType

Natural language names

Constants

Name | Description
--- | ---

CONSTANTVOLUME

| Constant Volume |

CONSTANTVOLUMESINGLEZONE

| Constant Volume Single Zone |

CONSTANTVOLUMEMULTIPLEZONEREHEAT

| Constant Volume Multiple Zone Reheat |

CONSTANTVOLUMEBYPASS

| Constant Volume Bypass |

VARIABLEAIRVOLUME

| Variable Air Volume |

VARIABLEAIRVOLUMEREHEAT

| Variable Air Volume Reheat |

VARIABLEAIRVOLUMEINDUCTION

| Variable Air Volume Induction |

VARIABLEAIRVOLUMEFANPOWERED

| Variable Air Volume Fan Powered |

VARIABLEAIRVOLUMEDUALCONDUIT

| Variable Air Volume Dual Conduit |

VARIABLEAIRVOLUMEVARIABLEDIFFUSERS

| Variable Air Volume Variable Diffusers |

VARIABLEAIRVOLUMEVARIABLETEMPERATURE

| Variable Air Volume Variable Temperature |

OTHER

| (other) | Value is not listed.

NOTKNOWN

| (unknown) | Value is unknown.

UNSET

| (unset) | Value has not been specified.

References: Pset_AirSideSystemInformation

Link to this page