IfcCableCarrierSegmentTypeEnum

BACnet MVD

#### IfcCableCarrierSegmentTypeEnum

Natural language names

| Cable Carrier Segment Type Enum
| Énumération des types de segment de chemin de cable

##### Semantic definitions at the type

Type definition

The IfcCableCarrierSegmentTypeEnum defines the range of different types of cable carrier segment that can be specified.

> HISTORY New type in IFC2x2.

Enumeration definition

Constant | Description
--- | ---
CABLELADDERSEGMENT | An open carrier segment on which cables are carried on a ladder structure.
CABLETRAYSEGMENT | A (typically) open carrier segment onto which cables are laid.
CABLETRUNKINGSEGMENT | An enclosed carrier segment with one or more compartments into which cables are placed.
CONDUITSEGMENT | An enclosed tubular carrier segment through which cables are pulled.
USERDEFINED | User-defined type.
NOTDEFINED | Undefined type.

##### Formal representations

XML Specification
`<xs:simpleType name="IfcCableCarrierSegmentTypeEnum">
<xs:restriction base="xs:string">
<xs:enumeration value="cableladdersegment"/>
<xs:enumeration value="cabletraysegment"/>
<xs:enumeration value="cabletrunkingsegment"/>
<xs:enumeration value="conduitsegment"/>
<xs:enumeration value="userdefined"/>
<xs:enumeration value="notdefined"/>
</xs:restriction>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcCableCarrierSegmentTypeEnum = ENUMERATION OF (
CABLELADDERSEGMENT,
CABLETRAYSEGMENT,
CABLETRUNKINGSEGMENT,
CONDUITSEGMENT,
USERDEFINED,
NOTDEFINED);
END_TYPE;

EXPRESS-G diagram

`

References: IfcCableCarrierSegment IfcCableCarrierSegmentType

Link to this page