IfcTemperatureGradientMeasure

BACnet MVD

#### IfcTemperatureGradientMeasure

Natural language names

| Temperature Gradient Measure
| Mesure de gradient de température

##### Semantic definitions at the type

Type definition

The temperature gradient measures the difference of a temperature per length, as for instance used in an external wall or its layers. It is usually measured in K/m.

Type: REAL

> HISTORY New type in IFC2x2.

##### Formal representations

XML Specification
`<xs:simpleType name="IfcTemperatureGradientMeasure">
<xs:restriction base="xs:double"/>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcTemperatureGradientMeasure = REAL;
END_TYPE;

EXPRESS-G diagram

`

References: IfcDerivedMeasureValue

Link to this page