Pset_DuctSegmentOccurrence

BACnet MVD

#### 7.5.4.39 Pset_DuctSegmentOccurrence

PSET_OCCURRENCEDRIVEN / IfcDuctSegment

Natural language names

| Duct Segment Occurrence

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

InteriorRoughnessCoefficient

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Interior Roughness Coefficient | The interior roughness of the duct fitting material.
| 内面粗さ係数 | ダクト継手材料の内面粗さ

HasLiner

P_SINGLEVALUE / IfcBoolean

| Has Liner | TRUE if the fitting has interior duct insulating lining, FALSE if it does not.
| 内張り有無 | 内貼り保温ダクト内面にあるときにTRUE。無い時にFALSE

Color

P_SINGLEVALUE / IfcLabel

| Color | The color of the duct segment. Note: This is typically used for any duct segments with a painted surface which is not otherwise specified as a covering.
| 色 | ダクト継手の色 メモ：塗装されているときに使用される。他の場合は仕上げとして定義

Link to this page